(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+3.3V")
	(net 2 "GND")
	(net 3 "Net-(DS1-SCK)")
	(net 4 "Net-(DS1-SDA)")
	(net 5 "+BATT")
	(net 6 "Net-(U3-OC)")
	(net 7 "unconnected-(Q1-Pad1)")
	(net 8 "Net-(U3-OD)")
	(net 9 "unconnected-(Q1-Pad1)_1")
	(net 10 "Net-(J3-Pin_4)")
	(net 11 "Net-(J3-Pin_3)")
	(net 12 "Net-(J3-Pin_5)")
	(net 13 "Net-(J3-Pin_2)")
	(net 14 "unconnected-(U1-GPIO4-Pad4)")
	(net 15 "unconnected-(U1-GPIO5-Pad5)")
	(net 16 "unconnected-(U1-GPIO6-Pad6)")
	(net 17 "Net-(BZ1-+)")
	(net 18 "unconnected-(U1-GPIO2-Pad2)")
	(net 19 "Net-(U2-~{CHRG})")
	(net 20 "Net-(U2-~{STDBY})")
	(net 21 "Net-(U2-PROG)")
	(net 22 "CHARGE+5V")
	(net 23 "unconnected-(U3-TD-Pad4)")
	(net 24 "Net-(U3-CS)")
	(net 25 "Net-(U3-VCC)")
	(net 26 "Net-(D1-K)")
	(net 27 "Net-(D2-K)")
	(net 28 "Net-(J2-CC2)")
	(net 29 "Net-(J2-CC1)")
	(net 30 "Net-(Battery1-Pin_1)")
	(net 31 "Net-(J1-Pin_3)")
	(net 32 "Net-(J1-Pin_2)")
	(footprint "OLED_128X64_1.3_I2C:LCD_OLED_128X64_1.3_I2C"
		(layer "F.Cu")
		(uuid "2364dc79-b1d7-4ed7-b853-bc4aef3de895")
		(at 203.2 71.6 180)
		(property "Reference" "DS1"
			(at -14.575 -17.885 0)
			(layer "F.SilkS")
			(uuid "d2764d41-6710-42d2-b51c-9307e6bb81bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "OLED_128X64_1.3_I2C"
			(at 0 -18.316 0)
			(layer "F.Fab")
			(uuid "30336d13-6264-44de-a2f2-14dd8d144775")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "16ad9662-abe9-419f-802a-ebb56dd855e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f3b811c-2e23-46f9-b8dd-d3886cd3a972")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "MF" "UNIVERSAL-SOLDER Electronics Ltd"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56a23bff-0993-43fe-b664-90e5599f937d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description_1" "Non-Touch Graphic LCD Display Module Transmissive White OLED, Monochrome I2C 1.3 (33.02mm) 128 x 64"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f8272709-b5ee-4ca7-8ebc-d6baea850570")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Package" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f61c8003-211b-41b8-8ff1-53fbfed88215")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7fdc8697-2ede-49a0-aa77-ef37820e8a77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/OLED%20128x64%201.3%22%20I2C/UNIVERSAL-SOLDER+Electronics+Ltd/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1ae0492a-6674-4c76-9533-7ac55422186c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c447c3a3-868e-4bff-acd6-5ed460d01bb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "PARTREV" "NA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "52bd6b6a-6ba3-4f3b-b2b5-dc7bca97f32c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/OLED%20128x64%201.3%22%20I2C/UNIVERSAL-SOLDER+Electronics+Ltd/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "608271a0-0c42-4a0a-ba1d-002f39932ad1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MP" "OLED 128x64 1.3&quot; I2C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bfa1a10-74eb-41aa-b8f3-bffc4e21a8ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Availability" "Not in stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56a64c24-b523-4637-927f-e635e24617e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MANUFACTURER" "UNIVERSAL-SOLDER Electronics Ltd"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f49b42bf-825a-4fe1-ae98-2a2654bcd08a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/a6e4f494-36b8-4f5d-9eaf-c6982777ca0a")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 17.75 16.85)
			(end -17.75 16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa1280c9-01e7-4b2d-b694-4a564a495e97")
		)
		(fp_line
			(start 17.75 -16.85)
			(end 17.75 16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd5d5826-89ef-4040-b0e7-60e41cf83804")
		)
		(fp_line
			(start -17.75 16.85)
			(end -17.75 -16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8119ff66-8c2c-4656-a908-a8beca91e795")
		)
		(fp_line
			(start -17.75 -16.85)
			(end 17.75 -16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8789353-5c47-49fb-9cb8-94d2d18d649b")
		)
		(fp_circle
			(center -3.81 -17.4)
			(end -3.71 -17.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "df9a9ac3-d7a2-4f05-8186-fbff2dbd32c0")
		)
		(fp_line
			(start 18 17.1)
			(end 18 -17.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79feb908-d7d4-4e96-856d-f316e88be9ca")
		)
		(fp_line
			(start 18 -17.1)
			(end -18 -17.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5bde248d-4f80-46ff-9ae1-cbfdedfca0fa")
		)
		(fp_line
			(start -18 17.1)
			(end 18 17.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17919f6c-97f9-4d6c-b8e6-6d273f37252f")
		)
		(fp_line
			(start -18 -17.1)
			(end -18 17.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbbb40b1-b51a-413a-b17f-238e7d75a5a4")
		)
		(fp_line
			(start 17.75 16.85)
			(end -17.75 16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c848a03a-2cd8-4be5-9221-ad94770a5d61")
		)
		(fp_line
			(start 17.75 -16.85)
			(end 17.75 16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "baa09b9e-72f0-4a27-9179-0d3e6e23d00f")
		)
		(fp_line
			(start -17.75 16.85)
			(end -17.75 -16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b13fd8ee-0428-4419-8bbe-de57235981e4")
		)
		(fp_line
			(start -17.75 -16.85)
			(end 17.75 -16.85)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a34d3383-f402-4f18-b75c-4ad699e8da50")
		)
		(fp_circle
			(center -3.81 -17.4)
			(end -3.71 -17.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ac46aaf3-7a17-46e1-b76b-a1572839bffa")
		)
		(pad "" np_thru_hole circle
			(at -15.75 -14.85 180)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(uuid "05ea0dab-db9c-490c-83c0-fffff9df4988")
		)
		(pad "" np_thru_hole circle
			(at -15.75 14.85 180)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(uuid "af317aaf-fd26-4b3c-b0db-b1afff1e947b")
		)
		(pad "" np_thru_hole circle
			(at 15.75 -14.85 180)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(uuid "4f50e40f-c8a4-4845-a2e7-73fd4afc9cb3")
		)
		(pad "" np_thru_hole circle
			(at 15.75 14.85 180)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(uuid "121b407f-9840-499d-bf80-29d1e781b854")
		)
		(pad "1" thru_hole rect
			(at -3.81 -15.55 180)
			(size 2.2 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "0c36afac-d9ae-4e23-b0c9-9beab1ad58ee")
		)
		(pad "2" thru_hole circle
			(at -1.27 -15.55 180)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "41fcd60b-bec9-49c0-8f54-66210d87efd0")
		)
		(pad "3" thru_hole circle
			(at 1.27 -15.55 180)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(DS1-SCK)")
			(pinfunction "SCK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "9b53b53c-658d-4d74-ba53-9ef5abbcf630")
		)
		(pad "4" thru_hole circle
			(at 3.81 -15.55 180)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(DS1-SDA)")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "f38f01c0-46f7-41d5-b645-3302a0f6eec7")
		)
		(embedded_fonts no)
	)
	(footprint "Buzzer_Beeper:Buzzer_15x7.5RM7.6"
		(layer "F.Cu")
		(uuid "303a4da9-1212-44b1-a680-70e4a2b59a8e")
		(at 199.41 75.692)
		(descr "Generic Buzzer, D15mm height 7.5mm with RM7.6mm")
		(tags "buzzer")
		(property "Reference" "BZ1"
			(at 3.81 -8.89 0)
			(layer "F.SilkS")
			(uuid "de95fb8c-b9c7-4360-a31c-4cd2579d3da8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Buzzer"
			(at 3.81 8.89 0)
			(layer "F.Fab")
			(uuid "6bf6126b-987c-4aea-a9a5-0b4c10aaf01f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0c008b1-4c42-4e22-ad48-312a39dd7c89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "93b1a4fb-b47e-418b-95ea-9e9a39657a94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Buzzer*")
		(path "/1a0f7142-9efc-4791-bf57-bf4d4ae3afd4")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 3.8 0)
			(end 11.4 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "442a64a6-be32-4adb-8271-cd1a514f06d0")
		)
		(fp_circle
			(center 3.8 0)
			(end 11.55 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "66d92f63-6325-4814-9c4e-ad19caa38412")
		)
		(fp_circle
			(center 3.8 0)
			(end 4.8 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "0a3c3eae-6a03-4bd9-b80d-fec1fb1fb0aa")
		)
		(fp_circle
			(center 3.8 0)
			(end 11.3 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8a907401-42d4-4095-ab65-c3b52201d333")
		)
		(fp_text user "+"
			(at -0.01 -2.54 0)
			(layer "F.SilkS")
			(uuid "e961c87b-01ff-4a2c-a3ed-49225c0d480f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "+"
			(at -0.01 -2.54 0)
			(layer "F.Fab")
			(uuid "06479f78-ab9a-4d6e-8881-64aabf651b3b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 3.8 -4 0)
			(layer "F.Fab")
			(uuid "c69eed50-8b6b-4db3-aee9-b14f5ff30815")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(BZ1-+)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "e46293af-1f84-41c0-86c1-774670ff8971")
		)
		(pad "2" thru_hole circle
			(at 7.6 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(uuid "fdfafbbe-b690-4c29-94bb-280d52387c5f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_15x7.5RM7.6.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "3a007b70-d872-4ebb-ae49-23bfbdd7d0d6")
		(at 192.278 141.224 180)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U3"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "334aaf19-e377-4ef8-b19b-d809cb39cc4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "DW01A"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "23d1fae8-ffd7-4833-962a-6d651cf86c32")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://hmsemi.com/downfile/DW01A.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ab11e7e-5b1a-4c4b-b6e6-22b2cc567aba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Overcharge, overcurrent and overdischarge protection IC for single cell lithium-ion/polymer battery"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6d022fe-ad87-4ddb-bb01-e44284f8e2ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/804c4dcb-7b01-443d-9be6-4ebba596536a")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.91 1.56)
			(end -0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e09cd60-d6e2-4538-a635-8ea1a60b5b6e")
		)
		(fp_line
			(start 0.91 1.51)
			(end 0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e762560-2d7d-472f-985e-a30f5381847f")
		)
		(fp_line
			(start 0.91 -1.56)
			(end 0.91 -1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2586cb0-00b0-4929-9e35-aa504eb92a55")
		)
		(fp_line
			(start -0.91 1.56)
			(end -0.91 1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e2e7eca-9f57-4572-9a38-d82b66c12dbd")
		)
		(fp_line
			(start -0.91 -1.51)
			(end -0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e78b2085-f7ff-4657-a95c-b359269e9411")
		)
		(fp_line
			(start -0.91 -1.56)
			(end 0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7dddd45d-6542-4934-872d-1759556165c2")
		)
		(fp_poly
			(pts
				(xy -1.45 -1.51) (xy -1.69 -1.84) (xy -1.21 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "21a61457-ebc8-45d1-8470-2083314ef203")
		)
		(fp_line
			(start 2.05 1.5)
			(end 1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecb06fdb-bc6b-4944-9f82-de84de7988e8")
		)
		(fp_line
			(start 2.05 -1.5)
			(end 2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40184b8f-e7ec-4a62-ade5-5876d7c8bec0")
		)
		(fp_line
			(start 1.05 1.7)
			(end -1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93ca4075-4df1-490e-a43f-0b77190a25e6")
		)
		(fp_line
			(start 1.05 1.5)
			(end 1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80854b61-e734-496f-8718-f6c6f3c409a7")
		)
		(fp_line
			(start 1.05 -1.5)
			(end 2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f7715ed-290a-43ce-a656-72f9746bde31")
		)
		(fp_line
			(start 1.05 -1.7)
			(end 1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c627a6b-ff6b-435a-8725-502d3732179c")
		)
		(fp_line
			(start -1.05 1.7)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa8b6a4b-fd7e-439f-8a7f-933aab624ae8")
		)
		(fp_line
			(start -1.05 1.5)
			(end -2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ceebe0bf-6d3e-44cc-858c-6d06d695394e")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d79cda37-3694-496a-9d2f-ea507695f78f")
		)
		(fp_line
			(start -1.05 -1.7)
			(end 1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "206ecad2-c68d-4719-97ea-bb43c541795b")
		)
		(fp_line
			(start -2.05 1.5)
			(end -2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3cfdbb9-84ac-43f6-b792-f424c301f40c")
		)
		(fp_line
			(start -2.05 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bf5d9d1-a6df-499a-9653-66157dd7cbad")
		)
		(fp_poly
			(pts
				(xy -0.8 -1.05) (xy -0.8 1.45) (xy 0.8 1.45) (xy 0.8 -1.45) (xy -0.4 -1.45)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ea46bac4-29ba-4ead-9088-8b199eac222f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "2a7191b2-d668-476e-a05a-15c019c563a5")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.11)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U3-OD)")
			(pinfunction "OD")
			(pintype "output")
			(uuid "ba2ff6d2-b0ed-4e02-8be2-2929d9018a18")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U3-CS)")
			(pinfunction "CS")
			(pintype "input")
			(uuid "c9b598ec-604b-4859-abd4-bddb0f4e5b07")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U3-OC)")
			(pinfunction "OC")
			(pintype "output")
			(uuid "fbc3e579-4c40-4ce0-b859-4fcae495903e")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "unconnected-(U3-TD-Pad4)")
			(pinfunction "TD")
			(pintype "no_connect")
			(uuid "2d49e5db-f874-417e-9047-e3404c5f5318")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U3-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "d8588850-49cf-4d5d-840b-f1edcaec54f2")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(Battery1-Pin_1)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "7cfc7a4b-dfce-42b4-af32-cfee997d3dad")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "412ea259-7cc2-4131-b974-a809fb74b280")
		(at 215.138 132.588 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(uuid "af20e6e5-2da4-46a0-82ff-937cfb9444b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.83 0)
			(layer "F.Fab")
			(uuid "1d90b383-426e-42d4-90b3-4c4c1e1994fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d81744d3-f8b6-4214-aaac-54e56a7cdb1c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "02fb32f4-91b9-439c-836c-2633c8d20afa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f8f9a6b-e5eb-42ac-8d35-547655dba868")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/10144ac1-5100-46dd-b69d-7056f6b8c537")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.6 -1.135)
			(end -2.46 -1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65343a1e-7dfc-4f43-9596-3d26255a13f4")
		)
		(fp_line
			(start -2.46 1.135)
			(end 1.6 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b2af84e7-d30c-45ae-9a8c-4642b066a29a")
		)
		(fp_line
			(start -2.46 -1.135)
			(end -2.46 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6742327-bce8-47ed-aa68-cfa9cb81c3e9")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1538ef11-b39c-4062-97a5-74c569242331")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ed893c9b-65ca-411b-b7a4-ba207a6ae3fa")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67cd5eba-64e6-4b23-bc90-372389ecaa6c")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de14d2d3-4346-4cf9-b9e5-2dab58cc54a2")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bcca9a6d-9394-471f-aa70-2a70076d331c")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.2 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c4b2ae9-01e7-4d7b-ad92-84c3d8020728")
		)
		(fp_line
			(start -1.2 -0.8)
			(end -1.6 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27ce23b7-4552-4365-a847-4bb48fdf1c1e")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "768740d5-7031-403f-b5b5-18e5a21bcd34")
		)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c163c925-6184-4b4a-ba47-1774b46b6514")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "619a34d8-012c-4c71-b3a8-4db178844f60")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.175439)
			(net 27 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "4f9461c4-01c0-4bc3-a5fd-a417f629a482")
		)
		(pad "2" smd roundrect
			(at 1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.175439)
			(net 22 "CHARGE+5V")
			(pinfunction "A")
			(pintype "passive")
			(uuid "a480573a-f6a8-4bce-8482-66e0e68f982d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "444b1d21-95e5-470b-8590-f0dcf9920ff0")
		(at 215.138 128.524 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(uuid "7d4dab2a-fe7e-4f5e-a9ea-015d82620cc2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.83 0)
			(layer "F.Fab")
			(uuid "a17b787e-db57-4492-83d3-a47ddcd51e9c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0fb4dffd-ada9-4c64-a595-54c1da449224")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea5e5479-3aaf-494a-90c3-1790f1391f8b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f82d1ca-0b63-4ffe-b481-bc0be8a56571")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/0945c013-f70d-4f17-980b-7b6e861e21d7")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.6 -1.135)
			(end -2.46 -1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17fb7e55-8a9e-4cbb-9408-9fca581d6512")
		)
		(fp_line
			(start -2.46 1.135)
			(end 1.6 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "919f3512-87be-440a-839e-e9157b12417c")
		)
		(fp_line
			(start -2.46 -1.135)
			(end -2.46 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a74f5fd-f371-4de3-8185-fe1d53775baf")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7833de3-7826-4f0c-8b8e-0c39c9e93d81")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d79fd740-9c11-4990-952a-9a8e1ffbcd70")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e22dbf1-5d9f-4cd6-9860-aee87ed6690f")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45b9fcc8-92b5-4d8e-8c82-ffb78f77e500")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b040378-9332-4669-8a3a-e34202359fde")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.2 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "574a1fc4-63cb-4cf1-b875-6a10a07d809e")
		)
		(fp_line
			(start -1.2 -0.8)
			(end -1.6 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdb500cb-c846-441e-abcf-2e89c644aab3")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "621d4e2b-a4a9-4e49-9a7c-1394868892c4")
		)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03a118ab-3324-45fb-8190-c429a6f61a4c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b3e78252-4b1f-4a37-abe4-008ee337a5ff")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.175439)
			(net 26 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "701985bb-c074-4d3a-b559-9ffe7475bc8a")
		)
		(pad "2" smd roundrect
			(at 1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.175439)
			(net 22 "CHARGE+5V")
			(pinfunction "A")
			(pintype "passive")
			(uuid "82d6342b-d1c9-4d1f-a595-7ad0f6d981f8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "61affb98-7bfa-41f9-82c0-ec44d08bab0a")
		(at 220.954 128.524 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(uuid "82846b7e-2183-426b-ba6f-17d78b8afce1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1K"
			(at 0 1.83 0)
			(layer "F.Fab")
			(uuid "27b21441-f291-4a2b-8c1a-eaeff0e60dcf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a16e8e0b-1419-41a6-bcd9-b14a6d2ad753")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0b17b7c-f06c-4575-a20f-cda0a1140244")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/69db3ef8-49a1-4a6b-b7a9-246517a8d68c")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d8c3a65-59a7-4fd3-85e5-50c003efc553")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b465ee00-f094-43ab-9cb4-6cc1c2a27cb1")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0812e45-bd65-497f-872b-66e0e0772c36")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7faeacf-2974-4461-9e44-cac7def0d42a")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0303d895-91a1-4feb-aec4-9865e8d9fb0e")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "814d0a51-e370-4ffd-aa2b-ddc758a1d683")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97782779-da17-4aa4-9d2b-86b7e4519b41")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b10cab58-6e20-406c-8808-5e771b0b6414")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45071617-a056-470a-8021-adb68fcbfa4b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d208583b-bab3-4425-9e01-45758c7d5cb6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f74ed5c8-3d4f-4fe2-83b8-d87bbd1fb174")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 20 "Net-(U2-~{STDBY})")
			(pintype "passive")
			(uuid "6e993ae8-7f46-4d7c-ad93-8a59f58f3986")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 26 "Net-(D1-K)")
			(pintype "passive")
			(uuid "9eff635f-efa6-4fb8-9731-e5905c686af4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "643dcbe5-205d-4802-8362-57134b41f1c5")
		(at 219.964 103.378 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J1"
			(at 2.54 0.254 0)
			(layer "F.SilkS")
			(uuid "97fd6941-e365-4c1a-bb28-2a030b677bbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "UART"
			(at 3.556 -1.27 0)
			(layer "F.Fab")
			(uuid "09db5eaf-d1c2-4f3d-8735-c014cb209840")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9d0ab7b-5c40-4bfe-ac75-d9fc4d72267a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "00ef2a45-1585-445e-a50a-614bf97f3e4f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/b33e06f9-1c41-4e22-9036-5876ac36e943")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.38 1.27)
			(end 1.38 6.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b28ac3b-6ac6-43d6-a68b-77c0eeb4546a")
		)
		(fp_line
			(start -1.38 6.46)
			(end 1.38 6.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6231e3a8-bb32-4a69-9ff2-645b9744d30b")
		)
		(fp_line
			(start -1.38 1.27)
			(end 1.38 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ffb57a0-e371-47f1-aab1-25289c20e252")
		)
		(fp_line
			(start -1.38 1.27)
			(end -1.38 6.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd59871b-fd01-4c0a-a750-e2c77d55c18f")
		)
		(fp_line
			(start -1.38 0)
			(end -1.38 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0051925-4b74-4ff3-8955-3b3473be401d")
		)
		(fp_line
			(start -1.38 -1.38)
			(end 0 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d78e7941-f7a0-4c25-90a4-2d0ab11509d4")
		)
		(fp_line
			(start 1.77 6.85)
			(end 1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7a98067-afce-49c8-9af5-12debac3bc3b")
		)
		(fp_line
			(start 1.77 -1.77)
			(end -1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa440087-8a56-449f-874b-97e28d900716")
		)
		(fp_line
			(start -1.77 6.85)
			(end 1.77 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "34321fa6-975b-4957-a63d-0c2f61815d7d")
		)
		(fp_line
			(start -1.77 -1.77)
			(end -1.77 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "573b7ee5-a21a-4ca4-8a96-3d83ef475aa9")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cae0b06e-463e-444e-8b88-332cdf1fbdab")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e44ff85-f9b3-430a-9116-a57637631e55")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4c08c43-eab9-45e8-912e-995a23e50ed0")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8289976c-4fce-41fa-97a9-6b80e73bf071")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3bd47e4e-228d-4e41-ae83-a9f694e426a4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "2a50f586-0d31-4622-a577-36fd23c4b937")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "e0cae046-4100-4e32-825a-1e966c3848ed")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "79e0946e-9720-4cc5-8328-534cea5d68af")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "57c13e3d-40d0-4ad4-8069-658d59eefc57")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_MEC_5GSH9"
		(layer "F.Cu")
		(uuid "6ec527d0-3f60-4e49-b525-4de6b406eff9")
		(at 203.2 101.6 90)
		(descr "MEC 5G single pole normally-open tactile switch")
		(tags "switch normally-open pushbutton push-button")
		(property "Reference" "SW1"
			(at -3.325 -8.575 90)
			(layer "F.SilkS")
			(uuid "312093e4-454d-4592-8f4e-7087ce670db3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_MEC_5G"
			(at 0.475 8.825 90)
			(layer "F.Fab")
			(uuid "cfab7d2b-8d7c-449f-bb72-b0ecd38c5e31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9cbd18cc-3a8c-4844-94e6-74f05104e228")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5727793a-ba9a-4e77-83d8-750d13a8fe04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW*MEC*5G*")
		(path "/01c9dba3-258a-4553-b970-54c10d16b56f")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start 5.25 -5.25)
			(end 5.25 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffce4bb5-ced2-4a1b-b1fb-a0d029e081fe")
		)
		(fp_line
			(start 4.7 -5.25)
			(end 5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf15a6ec-5534-4640-bdbc-d27e01b08c79")
		)
		(fp_line
			(start -4.7 -5.25)
			(end -5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3880abec-9bca-4b57-9f3d-b29f31929992")
		)
		(fp_line
			(start -5.25 -5.25)
			(end -5.25 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9089b095-fd88-49f0-8cf0-f12021a9f4d4")
		)
		(fp_line
			(start 5.25 5.25)
			(end 5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d85aabb-fb96-496c-8001-2313985be473")
		)
		(fp_line
			(start 4.7 5.25)
			(end 5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89815b0a-70a8-4768-a05b-2820ef671fb0")
		)
		(fp_line
			(start -4.7 5.25)
			(end -5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3dc11e0b-f6e3-4df9-a243-2dd98a45a5ed")
		)
		(fp_line
			(start -5.25 5.25)
			(end -5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b1d2981-2e17-490a-9607-8be0ed9b21f0")
		)
		(fp_line
			(start 5.3 -7.8)
			(end 5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8d04441-f685-4bc8-8d0c-e9bac638c7e9")
		)
		(fp_line
			(start -5.3 -7.8)
			(end 5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7002c5d3-3676-4f97-9605-a33715a28a29")
		)
		(fp_line
			(start 5.3 7.8)
			(end -5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd6feaf6-c06b-452a-b492-7c3905ee2654")
		)
		(fp_line
			(start -5.3 7.8)
			(end -5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "047dc420-991e-48ce-b360-9198e034293a")
		)
		(fp_line
			(start 5 -5)
			(end 5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a58ee938-04cd-4e0d-92ba-1f72d0787faa")
		)
		(fp_line
			(start -5 -5)
			(end 5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bab6e65-f7e2-4cb3-8475-b81854992a67")
		)
		(fp_line
			(start 5 5)
			(end -5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbf2bd99-eabc-4f2b-9eb2-ed2b5ed2c223")
		)
		(fp_line
			(start -5 5)
			(end -5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a410bcc-313e-435e-9dbb-78ed0f861c29")
		)
		(fp_circle
			(center -3.85 -4.3)
			(end -3.85 -4.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "4f1d9110-273b-4579-a733-cc57878517f7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "510cc398-a804-4182-bc35-8865aaf39578")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.81 -6.25 180)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "b34c358e-b4bc-4bd6-971b-8836e2add6f0")
		)
		(pad "2" smd rect
			(at -3.81 6.25 180)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "04645443-05c4-434d-be87-83e04d356088")
		)
		(pad "3" smd rect
			(at 3.81 -6.25 180)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(J3-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "efd6bc2f-8ac0-49eb-acac-1f9f010f470b")
		)
		(pad "4" smd rect
			(at 3.81 6.25 180)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(J3-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "61c515c0-378b-42ac-804b-451ddc29d7c1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_MEC_5GSH9.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_MEC_5GSH9"
		(layer "F.Cu")
		(uuid "7308134e-9c4b-4d49-98dc-70ddae785fbd")
		(at 218.2 116.6)
		(descr "MEC 5G single pole normally-open tactile switch")
		(tags "switch normally-open pushbutton push-button")
		(property "Reference" "SW2"
			(at -3.325 -8.575 180)
			(layer "F.SilkS")
			(uuid "6c1c8ed8-901f-4bde-8202-ce4ac83d2ed6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_MEC_5G"
			(at 0.475 8.825 180)
			(layer "F.Fab")
			(uuid "ade77b01-8f62-4786-a54c-a7b8283e284a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e4aa3b1-16fb-4d87-86a6-85582723a465")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6b70df95-0852-4601-99f2-dd3d49846bbe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW*MEC*5G*")
		(path "/bf4960d5-e295-41e2-a0ac-f20b990ac275")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -5.25 -5.25)
			(end -5.25 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93999713-249f-48c0-8af2-469e7c7628bd")
		)
		(fp_line
			(start -5.25 5.25)
			(end -5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3d1f961-bb4e-4576-947c-18d479d0cf53")
		)
		(fp_line
			(start -4.7 -5.25)
			(end -5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2fe4ab0e-cfc6-457e-a451-10ecf528ec73")
		)
		(fp_line
			(start -4.7 5.25)
			(end -5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d56ddf5-714b-42e2-bd0a-b901f42763c9")
		)
		(fp_line
			(start 4.7 -5.25)
			(end 5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50b54990-cd5d-4d9d-83d6-b0dc6341414d")
		)
		(fp_line
			(start 4.7 5.25)
			(end 5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94d5c823-3790-4ae7-bf9b-82cb218e6aaa")
		)
		(fp_line
			(start 5.25 -5.25)
			(end 5.25 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "767288a8-a181-404e-bf9f-9efab3b1beb2")
		)
		(fp_line
			(start 5.25 5.25)
			(end 5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00eea5d2-be9f-4b58-9ad7-732937bb712d")
		)
		(fp_line
			(start -5.3 -7.8)
			(end 5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dceb1edc-8f78-4907-ae9f-0cd5aafe3e1a")
		)
		(fp_line
			(start -5.3 7.8)
			(end -5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "914a91e3-16d7-4156-8375-967fec459b45")
		)
		(fp_line
			(start 5.3 -7.8)
			(end 5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56248d15-c871-4066-962d-3de601401232")
		)
		(fp_line
			(start 5.3 7.8)
			(end -5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2842028-5e2c-404e-b068-397e64444258")
		)
		(fp_line
			(start -5 -5)
			(end 5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6f6fd80-c9a4-42a2-b388-bda05f52d8fd")
		)
		(fp_line
			(start -5 5)
			(end -5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91dae96b-3931-4d51-8c2b-269d631caf37")
		)
		(fp_line
			(start 5 -5)
			(end 5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6660e883-1c1a-45f5-acd7-dc99014525d6")
		)
		(fp_line
			(start 5 5)
			(end -5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "899797c8-a84a-49cf-9bcf-1c2a1d668021")
		)
		(fp_circle
			(center -3.85 -4.3)
			(end -3.85 -4.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "6c2a0ee2-b789-4157-844a-c3cb0c3ad846")
		)
		(fp_text user "${REFERENCE}"
			(at -0.2675 0 0)
			(layer "F.Fab")
			(uuid "063bf73d-9cb6-4063-8672-7086ca3716b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.81 -6.25 90)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "46985ac4-15c8-4528-baed-773b030abf86")
		)
		(pad "2" smd rect
			(at -3.81 6.25 90)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "6d688704-436a-43bb-a656-a34aa311d885")
		)
		(pad "3" smd rect
			(at 3.81 -6.25 90)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(J3-Pin_3)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "4ddbf3b0-6770-4642-a4a5-f0c7e1178786")
		)
		(pad "4" smd rect
			(at 3.81 6.25 90)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(J3-Pin_3)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "6becf55c-a400-469a-834d-c1159a7b3542")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_MEC_5GSH9.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "94700b17-37a7-4e3e-891f-f5ab14fa8c29")
		(at 195.834 139.7 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.83 90)
			(layer "F.SilkS")
			(uuid "fb23221b-34f3-4969-8bb0-5a7c1e22524d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1K"
			(at 0 1.83 90)
			(layer "F.Fab")
			(uuid "fb0cb6d9-2f44-4568-8516-76d130322e67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec4f8a7d-e266-471e-8a9d-59f95acf6ea7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0cd4089f-0a06-4b7b-ab86-740468921617")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/241ed022-6dd6-4dbc-a0ef-d05192e3b452")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3557853-2bac-45c9-952d-ab99cecfa883")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "702ed2d8-876a-44a4-a84c-5e283ba78752")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "255b8d3a-2b92-4822-8315-5d53b1c5f717")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61e003f5-54cf-42e5-b477-d29ca0838d86")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cf5dbbe-fd08-418b-9cd1-9cba750d3acd")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "444702fa-ff61-4c62-8ad1-2dd23949a781")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29d443b4-4145-4551-ad8a-dc168d1a7a1a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d530a20d-c937-4db2-b454-cdf4f9b1c355")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3a564e1-c95c-423b-9ccf-51d4b73ed2d9")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5194c592-2434-4c3e-b46c-2ff33eb02c92")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "cfb39d46-e543-4cac-a6ea-9c4992cd41db")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "GND")
			(pintype "passive")
			(uuid "8a9966e6-610c-4b64-a899-9e886ace95f2")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 24 "Net-(U3-CS)")
			(pintype "passive")
			(uuid "ccbd147e-e048-4925-9f5b-2525893b104b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_MEC_5GSH9"
		(layer "F.Cu")
		(uuid "9990a953-ba7c-404d-ad71-55d950e56a1b")
		(at 188.2 116.6 180)
		(descr "MEC 5G single pole normally-open tactile switch")
		(tags "switch normally-open pushbutton push-button")
		(property "Reference" "SW4"
			(at -3.325 -8.575 0)
			(layer "F.SilkS")
			(uuid "2807eb75-88e6-4551-bcb4-6c1ee338f462")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_MEC_5G"
			(at 0.475 8.825 0)
			(layer "F.Fab")
			(uuid "25a0b8a9-95c7-4484-9595-b5a653e81af9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f3e3a87a-c044-467c-b5a4-329b837f67cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbd4c9bf-87e6-44bd-bf94-6d67791ab929")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW*MEC*5G*")
		(path "/a30ffbdc-f083-4be9-9e96-d3e3b60b6ec5")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start 5.25 5.25)
			(end 5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fae5f3b0-616d-4410-8885-35e1a964a8bb")
		)
		(fp_line
			(start 5.25 -5.25)
			(end 5.25 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "510f169a-9814-4138-9414-069ad756ee71")
		)
		(fp_line
			(start 4.7 5.25)
			(end 5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb1f2611-33c1-46bc-abfb-2b1c23cc5876")
		)
		(fp_line
			(start 4.7 -5.25)
			(end 5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2e287da-94ae-40fe-9979-46e69ef37b2d")
		)
		(fp_line
			(start -4.7 5.25)
			(end -5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c04f19dd-17c1-479a-a823-f168548a4b27")
		)
		(fp_line
			(start -4.7 -5.25)
			(end -5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e04e5c2-2660-4e5d-943a-84e0e4377605")
		)
		(fp_line
			(start -5.25 5.25)
			(end -5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26232769-80a1-4d85-a813-388a0b0b56cf")
		)
		(fp_line
			(start -5.25 -5.25)
			(end -5.25 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4bd49e71-11a6-47b1-8ed6-a20a03340c8e")
		)
		(fp_line
			(start 5.3 7.8)
			(end -5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "559ea3ac-dbf4-451e-b660-8fbe270cab4c")
		)
		(fp_line
			(start 5.3 -7.8)
			(end 5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11c9025e-bba1-48cb-8b9a-f430e1a09363")
		)
		(fp_line
			(start -5.3 7.8)
			(end -5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "66e3defb-16c5-476c-b999-ff217c1e8737")
		)
		(fp_line
			(start -5.3 -7.8)
			(end 5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3f779fd-5341-4557-a29a-a6febc33ffbb")
		)
		(fp_line
			(start 5 5)
			(end -5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04cfda51-fa45-4762-a4ef-488b82e7f46b")
		)
		(fp_line
			(start 5 -5)
			(end 5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c601b64a-f724-4a23-a9f5-3e9b66b31e99")
		)
		(fp_line
			(start -5 5)
			(end -5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc4dfecd-1257-4e5b-80bc-a56f950a2a10")
		)
		(fp_line
			(start -5 -5)
			(end 5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "089430f9-a93c-4f7b-987d-bd4a42e10808")
		)
		(fp_circle
			(center -3.85 -4.3)
			(end -3.85 -4.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "99a9717f-8468-4c4e-92b3-b42a5cd7327b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "aef890f4-24f6-484b-ac0b-2ba8220c1671")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.81 -6.25 270)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "4dd96ae5-c777-45ab-8e8a-e2422acaf717")
		)
		(pad "2" smd rect
			(at -3.81 6.25 270)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8758a39d-d7de-417e-887a-f0a690f4d1b6")
		)
		(pad "3" smd rect
			(at 3.81 -6.25 270)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(J3-Pin_5)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "3b3915e9-3681-43a6-870a-21d847acca8c")
		)
		(pad "4" smd rect
			(at 3.81 6.25 270)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(J3-Pin_5)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "96b40bea-4d1a-4731-85ff-62cf0834b639")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_MEC_5GSH9.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "a0299c09-4691-417b-a2bc-4b95a186d67b")
		(at 188.976 141.986 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(uuid "7ccfff2c-3f64-44ae-bb4b-c4d26fcae458")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(uuid "6d8899ee-87c8-4cb6-b58b-36f4a65aa445")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7452b01-43e5-4a86-b7e2-7a5a99a9ca39")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "adf0b745-f2d2-45a2-859d-d81029f1778f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/39220ff4-23c5-4927-b96d-b7cd840e3e15")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bde456b9-9718-4248-bd37-c2ae38524407")
		)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70e4217d-93a3-4b04-94d4-c388b6ae60cb")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49b431e8-443d-4b1b-a860-ae155bc807df")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff8921a6-1b92-4844-a350-d8ecdc200d90")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "754035d8-75b7-490a-b4f8-ef16a4627776")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8174942c-0f89-46fa-b39a-de7980487ac4")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6b4319e-447e-4346-968a-421fbb378114")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d947a28b-74aa-4141-8c96-b665d52b8265")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c58c647-6965-496f-bd01-e2085f4bce2e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb0a9b84-c5a5-44c5-bd4b-8dcea17ca0e2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "8d02022c-959c-4424-b0de-424f9b8975da")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 25 "Net-(U3-VCC)")
			(pintype "passive")
			(uuid "6eb77ad3-fd36-468c-9a69-c4e5d18073ee")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 30 "Net-(Battery1-Pin_1)")
			(pintype "passive")
			(uuid "810c901b-a3e9-4e85-994c-09fec32477fd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "a03d6589-9ca2-46e3-9385-38d07648dfa5")
		(at 205.232 114.554 -90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.38 90)
			(layer "F.SilkS")
			(uuid "f0545b84-3d80-46b0-bf8a-1b763f815e7d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 12.54 90)
			(layer "F.Fab")
			(uuid "dfab5cbc-8157-4ad5-9b0f-b0ace636ca33")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd9dc9dd-4b98-418a-acde-92b0407a2ebb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3f811e0-defa-4393-9df8-940488edf465")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/833beef3-5adc-4eea-a378-37fd32c5be50")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.38 11.54)
			(end 1.38 11.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4fb38bc-1d53-42e5-b976-6134ee0a449a")
		)
		(fp_line
			(start -1.38 1.27)
			(end -1.38 11.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd3d88b6-3ea3-4d13-ae87-08a9661524fa")
		)
		(fp_line
			(start -1.38 1.27)
			(end 1.38 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19921f1e-603c-4574-9bec-850b29c0936e")
		)
		(fp_line
			(start 1.38 1.27)
			(end 1.38 11.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64f5bd26-6b03-47f0-9908-f85a874cff5b")
		)
		(fp_line
			(start -1.38 0)
			(end -1.38 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5088654e-33ce-4151-a7fb-e8964aa5c981")
		)
		(fp_line
			(start -1.38 -1.38)
			(end 0 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89e2672e-7fec-4dae-89bf-7704e37fa6de")
		)
		(fp_line
			(start -1.77 11.93)
			(end 1.77 11.93)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57b6b3e2-5114-4d99-9358-f13ef7ee32e0")
		)
		(fp_line
			(start 1.77 11.93)
			(end 1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41b6fc7c-63fe-417b-a4aa-4d5930879119")
		)
		(fp_line
			(start -1.77 -1.77)
			(end -1.77 11.93)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1aaf12d4-4336-43e3-8d41-faa9da87071f")
		)
		(fp_line
			(start 1.77 -1.77)
			(end -1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df46b786-6716-43ac-8b56-df02cbd5a847")
		)
		(fp_line
			(start -1.27 11.43)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b89447d0-db84-4460-909a-171bc585681b")
		)
		(fp_line
			(start 1.27 11.43)
			(end -1.27 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4aff8561-328b-41f7-aff9-a17b513de530")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dddeaca4-472c-4e6c-aa70-b66a874106a3")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a73d79c3-ee9c-45bc-8726-513f6c528cff")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0fc4396-4092-4a5e-8444-7c4256812b48")
		)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 0)
			(layer "F.Fab")
			(uuid "4f69fd07-7489-420e-b859-29de9801293a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.2 2.2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "d71b0dd3-7c8f-4da8-ad94-77604dbde7c3")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "ea9ced91-05e0-44ce-9cc0-8362a29be95d")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "72af3538-896d-4290-9fca-6380d3397d83")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "2f7ca333-179d-4aad-8410-e54c2ca25447")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "8764f473-0c83-4cc8-bba6-b07d959d5af8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_MEC_5GSH9"
		(layer "F.Cu")
		(uuid "a58e6b89-f02f-4e65-b6d0-4f6f4aaff26e")
		(at 203.2 131.6 -90)
		(descr "MEC 5G single pole normally-open tactile switch")
		(tags "switch normally-open pushbutton push-button")
		(property "Reference" "SW3"
			(at -3.325 -8.575 90)
			(layer "F.SilkS")
			(uuid "647dee25-d7dd-456f-8e36-8ebdba369eac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_MEC_5G"
			(at 0.475 8.825 90)
			(layer "F.Fab")
			(uuid "fbb22497-196c-4363-9221-3fba9e22aee3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44c9c4b3-9cdf-41a3-9319-e974aa729609")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c22dc1b4-af13-4905-91d2-a80c36adabcc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW*MEC*5G*")
		(path "/7f6c1f09-f1ad-48e6-b5df-bed0203c3fff")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -5.25 5.25)
			(end -5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6a4c895-f05a-4b10-921d-614569f5d01c")
		)
		(fp_line
			(start -4.7 5.25)
			(end -5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "645a33e8-c55f-473d-b1af-5e8b003ae351")
		)
		(fp_line
			(start 4.7 5.25)
			(end 5.25 5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5cbcec8-5548-438b-bdbe-a1dafd605eee")
		)
		(fp_line
			(start 5.25 5.25)
			(end 5.25 4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "85ebd42d-da35-47c8-b9ab-cf12881df5f7")
		)
		(fp_line
			(start -5.25 -5.25)
			(end -5.25 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91b3a36b-7b2f-4b3f-bd1d-dd9f61c886cf")
		)
		(fp_line
			(start -4.7 -5.25)
			(end -5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "263f44ce-4aee-425c-9236-32acb68e3858")
		)
		(fp_line
			(start 4.7 -5.25)
			(end 5.25 -5.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43734ec4-0efe-4c73-96e9-c1cb63d295cc")
		)
		(fp_line
			(start 5.25 -5.25)
			(end 5.25 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71c77ecb-0e6c-4f7c-b933-e1f221e5b9e7")
		)
		(fp_line
			(start -5.3 7.8)
			(end -5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd65d3a1-e67f-4675-8f40-d2a618a94695")
		)
		(fp_line
			(start 5.3 7.8)
			(end -5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "942e648f-0b96-4b50-b53a-d883bf7e5416")
		)
		(fp_line
			(start -5.3 -7.8)
			(end 5.3 -7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4d62ee0-ef94-4680-9ed6-3c7a97640b84")
		)
		(fp_line
			(start 5.3 -7.8)
			(end 5.3 7.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55e460d7-5706-41d1-8e1c-71ae79992cab")
		)
		(fp_line
			(start -5 5)
			(end -5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b80072f-960a-47a9-a3df-690f6793ef3d")
		)
		(fp_line
			(start 5 5)
			(end -5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7ba02b2-62a6-4770-b57e-7f378a439e55")
		)
		(fp_line
			(start -5 -5)
			(end 5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39c6dd7a-1959-4c1d-91fe-75c8e34b29ea")
		)
		(fp_line
			(start 5 -5)
			(end 5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4929ef34-1125-4dc8-93fb-0172cd0d58f8")
		)
		(fp_circle
			(center -3.85 -4.3)
			(end -3.85 -4.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5d2e7e1f-321e-4086-acd8-487ede5d2c27")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "245bd0d9-ff15-473d-88bd-2c28d8b67e4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.81 -6.25)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "1ec207d5-5fb9-4a49-912b-d04eedbde63d")
		)
		(pad "2" smd rect
			(at -3.81 6.25)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "49a08f8a-aacb-4e13-abd5-07a3314927f2")
		)
		(pad "3" smd rect
			(at 3.81 -6.25)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J3-Pin_4)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "a020b25a-2ecf-47a1-be19-c690068d50d0")
		)
		(pad "4" smd rect
			(at 3.81 6.25)
			(size 2.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J3-Pin_4)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "c389b5bd-9e11-4df5-a073-cf2078580f35")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_MEC_5GSH9.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "b5126ce1-e8ab-45ad-935b-9b4e2bb76cb3")
		(at 210.566 139.726 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -0.026 -1.778 90)
			(layer "F.SilkS")
			(uuid "30504e4b-333e-4e5a-8d90-088e5ecb0835")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.2K"
			(at 0 1.83 90)
			(layer "F.Fab")
			(uuid "6abfa14a-e280-4c30-ac74-f517fc972dfd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "79c19f9c-d722-4cef-a2ab-70f966e47b8d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b0cd6ef-886f-4647-9704-392f556c8e45")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/84621480-417b-4826-8769-1d022619a433")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f70e903-de68-4252-8cea-8a74775c6ead")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c68a54e-189b-4938-9ffd-1892bb7ddbf5")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06b2a8b9-f48c-4952-b4a1-460c9880a700")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ee92f21-ac50-4615-960b-8c09f267601e")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0fd0ad42-4606-41e3-88d8-3a7f977281d0")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "645ce26e-5afe-4499-8771-350adafe5238")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "154fba44-3db0-4864-8244-86b8c70d8ab9")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84c6ef1c-de59-4969-a866-641c6ca7fec0")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ec8185c-4bfa-4b0d-9907-d3b3bbf21bb6")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b29c645-769f-4685-9ca0-2f9031539d0f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "da24b486-c568-4828-a78a-be9d1c9846e9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 21 "Net-(U2-PROG)")
			(pintype "passive")
			(uuid "84b00d89-baea-4d79-8fa9-77c54de4b284")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "GND")
			(pintype "passive")
			(uuid "834a7940-d768-42d6-9cd9-0b43fd64fd77")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "cbf7da98-0e93-437a-a2d7-87a97ec020b0")
		(at 220.98 132.588 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(uuid "ab32cce2-3bea-45bb-8fc7-c9598ef5c83c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1K"
			(at 0 1.83 0)
			(layer "F.Fab")
			(uuid "a8d88168-7983-44e8-ab35-f577a2b76cfe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "70ba32dd-cfc9-4bf4-bc8d-8c70f35f5da7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1bab267-57cd-4e1c-8dad-445e0ed1b0b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/28c6b270-314f-438f-be0f-83a372c2ff6b")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7690a757-307e-4c44-a9f8-2f376562e1bd")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0948f2cc-ac2d-4c6e-98b8-be840fdf94c5")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8b649ca-eb9d-4bee-a7b6-419415496f3d")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ada0d094-aee7-49cf-9ba6-40dc9de72202")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "028e4978-4fcf-48ca-b4a0-c17918f25e46")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8321d33d-8b9b-4524-b78b-01ab62c3bfe8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f52ac49a-86c4-4127-b6c4-fd2a0f9ee8a9")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "750be671-bbd6-4538-bd68-8a5145fb569f")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13c5dbca-efc7-421e-b915-f8e3db08fcf9")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6afb77ff-8b12-4493-8162-16abf704c658")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8946f9aa-cacf-4c57-81d8-a5d9aaaa790f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 19 "Net-(U2-~{CHRG})")
			(pintype "passive")
			(uuid "7527b4c6-49e7-47d1-b2ed-dc6d3f58c7ad")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 27 "Net-(D2-K)")
			(pintype "passive")
			(uuid "b7831153-0df4-42ae-96fe-4d5d2011345d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "FS8205A:SOP65P640X120-8N"
		(layer "F.Cu")
		(uuid "d4733e70-0589-4afb-b5d8-4703d0fb4c6f")
		(at 185.674 140.97 90)
		(property "Reference" "Q1"
			(at -0.635 -2.327 90)
			(layer "F.SilkS")
			(uuid "f1d3e9e3-3b67-45b7-9abf-2cecf3151d11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FS8205A"
			(at 6.35 2.327 90)
			(layer "F.Fab")
			(uuid "272f5439-c932-464c-b5ff-b2c3d42f79a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0410ecf0-9e6d-4d79-a8d8-05463dc61f85")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "608c91e8-5819-4508-bd81-1e13cd382fc2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "MF" "Fortune Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0313463-d70e-438c-a879-64356610c25a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.2mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7efd424e-92f2-4fd9-85a7-c2707a961494")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Package" "Package"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7aa8f915-e1dc-4ada-8e37-054a5124b615")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "006d67b2-fb0f-49ab-9646-27198ac60927")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/FS8205A/Fortune+Semiconductor/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "498bfa0c-df3e-40ca-952a-12baf09f0962")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e183190-16e8-4992-9719-86d242a9da5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "PARTREV" "1.7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9b2b765-a24e-47ed-afcc-d94cce6b45f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/FS8205A/Fortune+Semiconductor/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ead01875-bb98-4141-a43b-81f0297baf4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MP" "FS8205A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4cd1fda-9292-4016-880d-79f4da780bd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description_1" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0f750cb-2735-4875-861f-b526d3c3637d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "923ef30d-5539-4b16-976f-b464ba85e813")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MANUFACTURER" "Fortune Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "afcf3e55-fddf-441f-87da-9db795f60a23")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/f074a379-9836-462f-b31b-69170432b566")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.25 -1.515)
			(end 2.25 -1.515)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cd7612f-bcf0-425e-b3ad-1b8a48d33c2d")
		)
		(fp_line
			(start -2.25 1.515)
			(end 2.25 1.515)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a267f7a-ffdb-40bd-8d9b-2ce0843d7998")
		)
		(fp_circle
			(center -4.44 -1.375)
			(end -4.34 -1.375)
			(stroke
				(width 0.2)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "9cb58472-fcdb-46e9-8ff5-6b4b6be6e3df")
		)
		(fp_line
			(start 3.91 -1.765)
			(end 3.91 1.765)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51626d76-1348-4d9c-a52b-fe0ede0479fc")
		)
		(fp_line
			(start -3.91 -1.765)
			(end 3.91 -1.765)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e8b8a1b-d422-4ce1-a997-53960bd3f14d")
		)
		(fp_line
			(start -3.91 -1.765)
			(end -3.91 1.765)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3041bfd-dcbd-4c8e-a1ba-4758dd203da9")
		)
		(fp_line
			(start -3.91 1.765)
			(end 3.91 1.765)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28359e82-1c66-49a3-9e2d-498586ba36fb")
		)
		(fp_line
			(start 2.25 -1.515)
			(end 2.25 1.515)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f99932a-2e71-442d-8bbe-656301c0614d")
		)
		(fp_line
			(start -2.25 -1.515)
			(end 2.25 -1.515)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c3fcee3-c9b4-499f-aecf-f864468ed88c")
		)
		(fp_line
			(start -2.25 -1.515)
			(end -2.25 1.515)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be46a5a4-6dd1-41f6-a015-0817d82c74a7")
		)
		(fp_line
			(start -2.25 1.515)
			(end 2.25 1.515)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43c86136-1b76-49bb-a4cd-a7a44a9d940c")
		)
		(fp_circle
			(center -4.44 -1.375)
			(end -4.34 -1.375)
			(stroke
				(width 0.2)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "aa022e45-8472-44cd-a17e-3f96b860b145")
		)
		(pad "1" smd roundrect
			(at -2.88 -0.975 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 7 "unconnected-(Q1-Pad1)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(uuid "976d427a-3cbd-4c7e-a511-798180d0b693")
		)
		(pad "2" smd roundrect
			(at -2.88 -0.325 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 30 "Net-(Battery1-Pin_1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "14c19617-32db-461e-81fd-6947595c4591")
		)
		(pad "3" smd roundrect
			(at -2.88 0.325 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 30 "Net-(Battery1-Pin_1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "878b129e-64aa-4504-913f-6cce738bc9b0")
		)
		(pad "4" smd roundrect
			(at -2.88 0.975 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 8 "Net-(U3-OD)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "c165fbec-629b-47b5-b0df-fb3604e4731d")
		)
		(pad "5" smd roundrect
			(at 2.88 0.975 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 6 "Net-(U3-OC)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "4fb2563e-8dc3-444b-80b1-aa5a0ffffb99")
		)
		(pad "6" smd roundrect
			(at 2.88 0.325 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 2 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "19e163fc-2d61-44a1-b452-3bd2075ebb2c")
		)
		(pad "7" smd roundrect
			(at 2.88 -0.325 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 2 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "7fc1fa36-8508-4def-8cb6-52b048705bfc")
		)
		(pad "8" smd roundrect
			(at 2.88 -0.975 90)
			(size 1.56 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 9 "unconnected-(Q1-Pad1)_1")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(uuid "e2d2a331-8013-4534-9e83-3ff92605a2da")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "ec75f947-475d-4fb8-9d9e-a16f2365b712")
		(at 192.05 138.176 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(uuid "a1ad625d-2c8f-4f95-af8c-2203df0d584e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100"
			(at 0 1.83 0)
			(layer "F.Fab")
			(uuid "0d3c6f94-715c-4515-9a40-45808a9df472")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8200750-fe42-43af-b832-eb63d14877af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "188f6a67-399f-4e3d-805f-3741d3077a94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1b87c954-0fb6-4f29-a4b2-58ea92e99f46")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7163a57e-b611-4394-bff0-e63c2fb7468e")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9234eba-7146-40c2-b4e4-51746e95a8fc")
		)
		(fp_line
			(start 2.45 1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03311d3a-022e-413e-88e4-e2d57cb32cea")
		)
		(fp_line
			(start 2.45 -1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a64b251-ea41-4f0d-b2bd-67c5fe0ee155")
		)
		(fp_line
			(start -2.45 1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fae4c7e3-9347-4dff-b0d0-2e06c5f68c7d")
		)
		(fp_line
			(start -2.45 -1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ea45f84d-dc46-4efd-a772-b287bbb7f26a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42b76695-023e-47c8-bcb7-0b1f27441ac6")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "136f5a25-bc25-4cda-b385-97d05572afa9")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec0f9483-305b-4572-9369-612d52cbf356")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc3b9ff2-009b-4bac-8cfb-04fcec9ace03")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d4c7389a-d42f-4451-b494-1099ec71115a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 5 "+BATT")
			(pintype "passive")
			(uuid "fb452956-2dca-49f1-a920-c768058af89c")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 25 "Net-(U3-VCC)")
			(pintype "passive")
			(uuid "cfb50d4b-6538-4fd3-b965-5ffe632f20ad")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm_ThermalVias"
		(layer "F.Cu")
		(uuid "f75906c7-11e1-4d0d-ad45-1c6dc85b64ae")
		(at 216.854 139.884)
		(descr "SOIC, 8 Pin (http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx#page=8), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "e27173b9-1d3f-4d28-b2f5-39e23f4b7c7d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TP4056-42-ESOP8"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "4d8b14fd-bcee-494b-b72c-db50ef5cfc03")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2410121619_TOPPOWER-Nanjing-Extension-Microelectronics-TP4056-42-ESOP8_C16581.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "78feebd3-0e62-4dc4-a63c-5e8feed672ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1A Standalone Linear Li-ion/LiPo single-cell battery charger, 4.2V ±1% charge voltage, VCC = 4.0..8.0V, SOIC-8 (SOP-8)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4e6337a-225e-4a02-b592-62301376a0a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*SO*3.9x4.*P1.27mm*EP2.4*x3.3*mm*")
		(path "/2057fe76-26ed-43df-a870-e19d13aae489")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.06 -2.56)
			(end 2.06 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9eb76015-ce64-4e3e-8b93-ad204fb21e57")
		)
		(fp_line
			(start -2.06 -2.465)
			(end -2.06 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffe56cca-5825-4b73-8190-2a6cc830502c")
		)
		(fp_line
			(start -2.06 2.56)
			(end -2.06 2.465)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8f8b2bb-173e-4af3-9497-813b09de464e")
		)
		(fp_line
			(start 2.06 -2.56)
			(end 2.06 -2.465)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24e89a0c-aaca-40ed-9256-825583e5df5e")
		)
		(fp_line
			(start 2.06 2.465)
			(end 2.06 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e03e3b28-a511-488e-a021-49d2abc69cf6")
		)
		(fp_line
			(start 2.06 2.56)
			(end -2.06 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "363d99ac-faa7-4d48-bf59-d90f3a076a0e")
		)
		(fp_poly
			(pts
				(xy -2.6 -2.47) (xy -2.84 -2.8) (xy -2.36 -2.8)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "91d31bc2-c81b-4493-a5e4-cde213c30e8c")
		)
		(fp_line
			(start -3.7 -2.46)
			(end -2.2 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a591e13a-cf3e-438d-96a8-f106477da291")
		)
		(fp_line
			(start -3.7 2.46)
			(end -3.7 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09ff8a4e-7005-4931-b95c-8ad68c344b38")
		)
		(fp_line
			(start -2.2 -2.7)
			(end 2.2 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22d71312-d238-4ba7-b8f8-396417d36259")
		)
		(fp_line
			(start -2.2 -2.46)
			(end -2.2 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa98a98f-7214-49ff-8687-3bb730fa62a6")
		)
		(fp_line
			(start -2.2 2.46)
			(end -3.7 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ea04d42-3de5-4d5e-8e64-2cc1808ddc76")
		)
		(fp_line
			(start -2.2 2.7)
			(end -2.2 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "69338e7f-f822-4841-962b-9bdf02f42599")
		)
		(fp_line
			(start 2.2 -2.7)
			(end 2.2 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07fd88e4-4ef0-4ddf-82d8-3ed614c6cbce")
		)
		(fp_line
			(start 2.2 -2.46)
			(end 3.7 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb67a468-45ea-406b-ae3a-764ca3f968a8")
		)
		(fp_line
			(start 2.2 2.46)
			(end 2.2 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "104b9ea4-86ae-4812-a308-5a72a67158ee")
		)
		(fp_line
			(start 2.2 2.7)
			(end -2.2 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09b3eae8-6096-42f5-b461-bb3a6d4abbe6")
		)
		(fp_line
			(start 3.7 -2.46)
			(end 3.7 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "297815ac-a581-4f9d-9c12-72a8c1f6b62b")
		)
		(fp_line
			(start 3.7 2.46)
			(end 2.2 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "443cf70f-abfb-4367-b8d2-839cefa38e6c")
		)
		(fp_poly
			(pts
				(xy -1.95 -1.475) (xy -1.95 2.45) (xy 1.95 2.45) (xy 1.95 -2.45) (xy -0.975 -2.45)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "beae0934-21b8-4158-b6f7-89aac1a6886d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7cee2f8b-16dc-47b9-b6cb-3ca164baf4fc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.6 -0.825)
			(size 1.01 1.38)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
			(uuid "de6be6e7-269d-4c42-868c-65542a085232")
		)
		(pad "" smd roundrect
			(at -0.6 0.825)
			(size 1.01 1.38)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
			(uuid "a6acb6ab-fefd-4acc-9c5d-629da4ea6b8a")
		)
		(pad "" smd roundrect
			(at 0.6 -0.825)
			(size 1.01 1.38)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
			(uuid "f647cd9c-4cbf-4fb4-a4c5-52901fece421")
		)
		(pad "" smd roundrect
			(at 0.6 0.825)
			(size 1.01 1.38)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
			(uuid "a619aca3-d39c-4a05-a66f-be94653f492d")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "TEMP")
			(pintype "input")
			(uuid "07bfa6b7-b344-4b61-b751-100665acab24")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U2-PROG)")
			(pinfunction "PROG")
			(pintype "passive")
			(uuid "734f1810-8125-4231-848c-2bbaef72c371")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "876401c1-8d28-40c4-bc99-63f48747c09a")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "CHARGE+5V")
			(pinfunction "V_{CC}")
			(pintype "power_in")
			(uuid "8016ec2e-45bb-4300-827f-735e86e88953")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+BATT")
			(pinfunction "BAT")
			(pintype "power_out")
			(uuid "158f6339-cf46-4946-8d2e-13fb71e0bec1")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-~{STDBY})")
			(pinfunction "~{STDBY}")
			(pintype "open_collector")
			(uuid "0d647e45-29f0-47dd-acf5-477e71b18173")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U2-~{CHRG})")
			(pinfunction "~{CHRG}")
			(pintype "open_collector")
			(uuid "02cea66c-2704-4c1b-ade1-dadd5c6c21fe")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "CHARGE+5V")
			(pinfunction "CE")
			(pintype "input")
			(uuid "a09d7806-2bab-4afa-a139-4dea483778d0")
		)
		(pad "9" thru_hole circle
			(at -0.7 -1.2)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(uuid "e1aa6df5-bee6-4fcf-b9cf-4232e4c15ad7")
		)
		(pad "9" thru_hole circle
			(at -0.7 0)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(uuid "1390499d-91e4-47cd-9219-640da35d389b")
		)
		(pad "9" thru_hole circle
			(at -0.7 1.2)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(uuid "f65545a9-1614-435b-8a0a-65fc7031ca1c")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 1.9 2.9)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(zone_connect 2)
			(uuid "8820b20c-fecc-4532-9317-97e5d33f7690")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 2.41 3.3)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(zone_connect 2)
			(uuid "dfb210fe-2c4b-4ed3-9aed-b52e03dcd343")
		)
		(pad "9" thru_hole circle
			(at 0.7 -1.2)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(uuid "b9bf5fe4-6994-4d0d-8e81-37f0fc16be28")
		)
		(pad "9" thru_hole circle
			(at 0.7 0)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(uuid "84681970-b195-41f6-bb93-ddde5b1e6348")
		)
		(pad "9" thru_hole circle
			(at 0.7 1.2)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EPAD")
			(pintype "passive")
			(uuid "cfcc6470-230c-46fa-9319-b92448531bfe")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(uuid "0e043b32-11a2-4917-b310-e2514e604cce")
		(at 200.66 135.382 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 1.83 0)
			(layer "B.SilkS")
			(uuid "b9b59e99-e650-4e0d-8a7d-8efec7067219")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "5k1"
			(at 0 -1.83 0)
			(layer "B.Fab")
			(uuid "57db8737-5fed-4a71-8968-5dc08fe78c27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "b2c58874-e223-4a7b-924d-48ebcac7149b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "38734bd0-f553-4922-9c00-140a7bda3c93")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/88d3602d-33c4-452d-922a-992faf57e1ea")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "88dcfc16-9d8f-47e5-9c8a-1176057127d5")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e153ff65-c9ef-475b-8a4a-1a280a0f627a")
		)
		(fp_line
			(start 2.45 1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "818c5336-52a0-46cb-9b84-f316d849c31c")
		)
		(fp_line
			(start 2.45 -1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0d464aa9-3dc4-4884-bff2-e0b87e2ca0b6")
		)
		(fp_line
			(start -2.45 1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2fd193ab-c216-4748-a054-b26cbfbd9998")
		)
		(fp_line
			(start -2.45 -1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0aa9c7fa-5c56-41b0-b977-d1f6f31357b7")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fac23614-2a54-401f-b1e3-559f531ec450")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "604c456c-1391-4910-a23b-a954bf99b0ff")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "278458c1-f07f-42c9-98e1-3ae72b17cebf")
		)
		(fp_line
			(start -1.6 -0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1a4bc8bb-30ac-4ff6-b0ba-630b1d610816")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "18b48cd5-ad1d-429d-bc72-852a7bdd9a8a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 28 "Net-(J2-CC2)")
			(pintype "passive")
			(uuid "8030fda1-8846-4568-89e0-9bcfe9508691")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "GND")
			(pintype "passive")
			(uuid "6a531e52-4504-4137-a931-857e95dd006a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ESP32-C3_SUPERMINI_SMD:MODULE_ESP32-C3_SUPERMINI"
		(layer "B.Cu")
		(uuid "0e435be0-ea7e-4f87-bcbf-428222a49a77")
		(at 195.834 114.554 -90)
		(property "Reference" "U1"
			(at -10.668 11.176 90)
			(layer "B.SilkS")
			(uuid "069b3044-21a8-4988-86f6-534fac805e4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "ESP32-C3_SUPERMINI_SMD"
			(at 6.985 -12.3825 90)
			(layer "B.Fab")
			(uuid "399e74bd-6577-420d-bde6-a67e1464d569")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "92a910b8-fdee-4511-b7a8-515104c830a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "b84cc46d-7136-47b3-8585-0f1ae2bf8d62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "MF" "Espressif Systems"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4bfe6df1-06e9-4268-82f0-110090f23531")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.2mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4b46e6af-bc1c-4aa1-807d-296902b74004")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "20ab117d-5269-4107-ae92-f1f2f3f6cb8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ff4b0198-d009-43b1-8cbb-b4c98c44338e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ESP32-C3%20SuperMini_SMD/Espressif+Systems/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a95748a7-c4d2-453a-a7b5-2f1b89593ced")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "df0e9db8-8a3b-46cb-95f7-a8ece4f9b938")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "PARTREV" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "17c8e7af-4475-4331-ac33-6e05fad58c8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32-C3%20SuperMini_SMD/Espressif+Systems/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "07515a6e-934f-4590-9f10-8aa0099f6c98")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "MP" "ESP32-C3 SuperMini_SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b030f7e5-21d1-47a6-84b8-97b02fad2d5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description_1" "Super tiny ESP32-C3 board"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "927b5bc8-9ef3-498a-b6e3-83f1e21d936c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Availability" "Not in stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "9d4f819c-6187-4fa1-b314-cef4f80a5555")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "MANUFACTURER" "Espressif"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "56cbab6f-b276-46ab-a75d-bbdc6744ac3d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(path "/ae3f7a54-cfa9-45db-9e01-b9629253c72c")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.5 12.65)
			(end -4.5 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "05a56754-2ebd-4fc8-8bfe-ccb8cc89fcd1")
		)
		(fp_line
			(start 4.5 12.65)
			(end -4.5 12.65)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e296fcd1-81f6-4359-bc1d-e84076fa9eac")
		)
		(fp_line
			(start 4.5 12.65)
			(end 4.5 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0f43bec5-893c-4590-b379-4954e845631f")
		)
		(fp_line
			(start -4.5 11.35)
			(end -9 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f05fe180-0f23-48c6-8d44-90da0a2af79c")
		)
		(fp_line
			(start 9 11.35)
			(end 4.5 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "55cfa182-3e13-4b29-a7ce-94e33a10bce8")
		)
		(fp_line
			(start -9 11.05)
			(end -9 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4f588775-3018-46e9-b490-1975eb08182d")
		)
		(fp_line
			(start 9 11.05)
			(end 9 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c9e99620-9a36-4d73-97da-02ec5baa171f")
		)
		(fp_line
			(start -9 -11.35)
			(end -9 -9)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b3aec0ca-cc10-4939-b156-df1414c56f7a")
		)
		(fp_line
			(start 9 -11.35)
			(end 9 -9)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8da43d23-5ff3-4dc5-b247-4e12ce432b90")
		)
		(fp_line
			(start 9 -11.35)
			(end -9 -11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0866b45d-3400-4031-8b5f-cdac67abb184")
		)
		(fp_line
			(start -9.7475 12.9)
			(end 9.7475 12.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e34fda13-e211-4fb4-bfb9-1cda63785434")
		)
		(fp_line
			(start 9.7475 12.9)
			(end 9.7475 -11.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1eb91758-70ea-425f-9395-c92be6dc10fc")
		)
		(fp_line
			(start -9.7475 -11.6)
			(end -9.7475 12.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c6ece801-a66d-4ef0-b7d5-c1424f12e775")
		)
		(fp_line
			(start 9.7475 -11.6)
			(end -9.7475 -11.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ea954ed0-a6ab-4e24-9e16-7ead308332d4")
		)
		(fp_line
			(start -4.5 12.65)
			(end -4.5 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9359fca4-c5ed-47e6-a905-23d63b347ea2")
		)
		(fp_line
			(start 4.5 12.65)
			(end -4.5 12.65)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "dd88fe5b-e995-4006-a878-406b8286fee5")
		)
		(fp_line
			(start 4.5 12.65)
			(end 4.5 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "27198559-0f91-4f73-be3d-fdc7e444bd03")
		)
		(fp_line
			(start -4.5 11.35)
			(end -9 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5cd5a28a-486d-4449-a72b-52e9ed9e2461")
		)
		(fp_line
			(start 9 11.35)
			(end 4.5 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "02c6ed8a-4e19-4be8-afdd-77d681b3cd0c")
		)
		(fp_line
			(start -9 -11.35)
			(end -9 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "478fb978-f52e-4040-a1ea-7c6f1be42f7a")
		)
		(fp_line
			(start 9 -11.35)
			(end 9 11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f58cb7ca-4e0f-4da5-bd83-47c5e540c9e1")
		)
		(fp_line
			(start 9 -11.35)
			(end -9 -11.35)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3e43ff1f-0530-4c51-9860-59f117efa182")
		)
		(pad "0" smd rect
			(at 7.985 -7.88 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "Net-(J3-Pin_2)")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "859b0c94-6a7b-4e57-8ec1-fffc86b9516b")
		)
		(pad "1" smd rect
			(at 7.985 -5.34 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "Net-(J3-Pin_3)")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "fe44f115-8f60-4350-869f-48dd681238ff")
		)
		(pad "2" smd rect
			(at 7.985 -2.8 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "unconnected-(U1-GPIO2-Pad2)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "be43f474-e2f3-466a-b395-f4caace46e70")
		)
		(pad "3" smd rect
			(at 7.985 -0.26 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(J3-Pin_4)")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "08279099-2cbd-43c5-8438-c6fc6680a213")
		)
		(pad "3.3" smd rect
			(at 7.985 4.82 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "+3.3V")
			(pinfunction "3V3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "725f4a4c-f590-4747-b044-53c442ea26d1")
		)
		(pad "4" smd rect
			(at 7.985 2.28 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "unconnected-(U1-GPIO4-Pad4)")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "359c8d9d-0e14-4caa-9d10-dd182ff7b8e1")
		)
		(pad "5" smd rect
			(at -7.985 9.9 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "unconnected-(U1-GPIO5-Pad5)")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "415d9807-e6da-4d09-b7dc-95b8b6efff79")
		)
		(pad "5V" smd rect
			(at 7.985 9.9 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "+BATT")
			(pinfunction "5V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "d50c1199-eed5-44ec-8b29-819d9349e7b5")
		)
		(pad "6" smd rect
			(at -7.985 7.36 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "unconnected-(U1-GPIO6-Pad6)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "858c2453-2aac-48a0-9077-72b87cf71aaf")
		)
		(pad "7" smd rect
			(at -7.985 4.82 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "Net-(BZ1-+)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "8f889bdf-253c-478f-afe1-d13002f39f7d")
		)
		(pad "8" smd rect
			(at -7.985 2.28 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "Net-(DS1-SDA)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "7ba8d7ae-945a-4ea4-b9e1-7a475a745ec8")
		)
		(pad "9" smd rect
			(at -7.985 -0.26 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "Net-(DS1-SCK)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "fbaec6e4-dfb7-4f9e-8dc5-6e67d1f8b170")
		)
		(pad "10" smd rect
			(at -7.985 -2.8 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "Net-(J3-Pin_5)")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "d0699aa5-96fc-4b41-8503-cb5ffefb8091")
		)
		(pad "20" smd rect
			(at -7.985 -5.34 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "Net-(J1-Pin_3)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "41d5faf1-e714-409e-99d7-4f8878ecc4f0")
		)
		(pad "21" smd rect
			(at -7.985 -7.88 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "Net-(J1-Pin_2)")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "025d6a7b-c500-4fd6-b067-76267afe3669")
		)
		(pad "G" smd rect
			(at 7.985 7.36 270)
			(size 3.025 1.524)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "c8fe8f8d-04a6-4bc5-aae0-d73cb9d3dec1")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4125-xx-x-0190_6P_TopMnt_Horizontal"
		(layer "B.Cu")
		(uuid "53138423-06dd-4bef-a922-3e111f2e22b7")
		(at 203.2 140.97 180)
		(descr "USB Type C Receptacle, GCT, power-only, 6P, top mounted, horizontal, 3A, 1.9mm stake: https://gct.co/files/drawings/usb4125.pdf")
		(tags "USB C Type-C receptacle power-only charging-only 6P 6C right angled")
		(property "Reference" "J2"
			(at 0 5.1 0)
			(unlocked yes)
			(layer "B.SilkS")
			(uuid "1457d7e0-9bb4-4afe-8517-49e5430aa5b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "USB_C_Receptacle_PowerOnly_6P"
			(at 0 -4.725 0)
			(unlocked yes)
			(layer "B.Fab")
			(uuid "e54daadd-5780-4ea2-a6af-fdf1643d389c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "fa760c11-897e-44e8-aff5-a430b2c5c786")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "USB Power-Only 6P Type-C Receptacle connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8f915c99-4566-48fc-a3f7-f9b887ff83a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(path "/394be4db-4a1d-4d4d-9a59-2e2feffaf317")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start 4.67 0.25)
			(end 4.67 1.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ab6752d6-64b9-4608-a589-b2ea1e505242")
		)
		(fp_line
			(start -4.67 0.25)
			(end -4.67 1.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6209ed60-9e88-4eb4-a9ee-6d303e30c59b")
		)
		(fp_line
			(start 5 -3.4)
			(end -5 -3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "c081ea75-fd3d-4093-9dd2-1692802d9baf")
		)
		(fp_rect
			(start -5.37 4.35)
			(end 5.37 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "d8706b50-b64b-47b7-a8e9-98aee121e352")
		)
		(fp_rect
			(start -4.47 3.4)
			(end 4.47 -3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "ab320c50-61a1-4055-85e2-7eca031e3107")
		)
		(fp_text user "PCB Edge"
			(at 0 -2.825 0)
			(unlocked yes)
			(layer "Dwgs.User")
			(uuid "27950a52-85f1-4b12-8f48-8d39d078ddbf")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0.275 0)
			(unlocked yes)
			(layer "B.Fab")
			(uuid "9fc9479c-92c9-4545-8e6c-d2ef23259b4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "A5" smd roundrect
			(at -0.5 3.08 180)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(J2-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(uuid "ccbb7d6b-c1f7-4c20-9f07-f122eab3f332")
		)
		(pad "A9" smd roundrect
			(at 1.52 3.08)
			(size 0.76 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "CHARGE+5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "710579de-53db-4165-b4ec-598bc9b3e323")
		)
		(pad "A12" smd roundrect
			(at 2.75 3.08)
			(size 0.8 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a4cfff48-e557-4628-aa7d-fb69cea34a7f")
		)
		(pad "B5" smd roundrect
			(at 0.5 3.08)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(J2-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(uuid "264db3b7-ea23-4d99-9c6d-3806aa5aa842")
		)
		(pad "B9" smd roundrect
			(at -1.52 3.08 180)
			(size 0.76 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "CHARGE+5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "92308846-fbd8-4c42-bb03-64918179cd32")
		)
		(pad "B12" smd roundrect
			(at -2.75 3.08 180)
			(size 0.8 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "744e6cc3-b72b-4014-8f2e-53fa0d0f3a13")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -0.8 180)
			(size 1.6 2.3)
			(drill oval 0.6 1.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "fc9966b5-da9a-4c1a-8c58-2fb760d1ff44")
		)
		(pad "S1" thru_hole oval
			(at -4.32 3 180)
			(size 1.6 2.3)
			(drill oval 0.6 1.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "4a419861-0162-485e-9a20-4d5195c22b61")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -0.8 180)
			(size 1.6 2.3)
			(drill oval 0.6 1.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "7770be84-0f8e-4bb1-aaa9-53c510219c1f")
		)
		(pad "S1" thru_hole oval
			(at 4.32 3 180)
			(size 1.6 2.3)
			(drill oval 0.6 1.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "3c0f2f51-c493-4eff-a666-ae875300eacb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4125-xx-x-0190_6P_TopMnt_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(uuid "5b1e2ed0-ed7d-4a32-a7f1-ee2ba270342d")
		(at 205.74 135.382)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 1.83 180)
			(layer "B.SilkS")
			(uuid "d727277a-f335-4fb9-a95d-0451d64c3057")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "5k1"
			(at 0 -1.83 180)
			(layer "B.Fab")
			(uuid "df93c47d-1ba2-4130-a3a6-a4c1dbe24f12")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "a2cdc8a0-40d7-42b4-86ab-3c3aae177e62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "f42c6468-fa60-4900-bccc-ec0cc1f474dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c1e04fa1-d497-4f5b-aa01-28be0b0aaf37")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "81f3355d-d86d-407d-81f0-807748cb0480")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3710d4a7-774a-4d81-93d4-4a4fbdbf5a55")
		)
		(fp_line
			(start -2.45 -1.13)
			(end -2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "82a7583d-23a0-440f-9622-e84a4063ab9b")
		)
		(fp_line
			(start -2.45 1.13)
			(end 2.45 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "edf05d0c-814d-47eb-9a53-6df7138065ce")
		)
		(fp_line
			(start 2.45 -1.13)
			(end -2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2b08a9f3-8252-44a1-87cd-7f13e5b48384")
		)
		(fp_line
			(start 2.45 1.13)
			(end 2.45 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ef123de2-416e-4aa3-84fe-578ba97680bd")
		)
		(fp_line
			(start -1.6 -0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c06550b2-6a97-4e65-bfd1-2a4f90125771")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "db0a19f0-eb2d-452c-a951-78d76289b0e3")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f1ccc450-ce41-4d10-8743-5bbda8a85418")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "37c8a6a3-6b7f-43cb-a314-6f4e751bfe37")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "51f4754c-3f4e-481f-9e03-6b0b86cd4370")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 29 "Net-(J2-CC1)")
			(pintype "passive")
			(uuid "50c78990-b4c2-4e76-ad8f-06ff3a8fa71d")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "GND")
			(pintype "passive")
			(uuid "2c67ea43-3072-490d-a72e-1e2121a3fe74")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S2B-EH_1x02_P2.50mm_Horizontal"
		(layer "B.Cu")
		(uuid "7cbd1788-28ee-49c6-b153-7c71a2bc4fde")
		(at 188.448 133.0885 180)
		(descr "JST EH series connector, S2B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "Battery1"
			(at 1.25 7.9 0)
			(layer "B.SilkS")
			(uuid "375fa80d-40b9-4769-bc29-401d427d26db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 -2.7 0)
			(layer "B.Fab")
			(uuid "1e32e0cf-0d7e-49a8-9eb4-651310df1cde")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "00df725b-e155-4b15-bb0c-7cf0dd23685c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "8e076b9c-925d-4f17-9e23-bfce52f2a0e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/b89b5b31-40f9-40b2-a18c-1296ca448484")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.11 6.81)
			(end 5.11 -1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7324ba85-7ec9-4919-bf79-9accadc89dd0")
		)
		(fp_line
			(start 5.11 5.59)
			(end 3.89 5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3db44f6d-eb0e-435f-b43d-43e676760fb9")
		)
		(fp_line
			(start 5.11 -1.61)
			(end 3.89 -1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "23d04212-c0e6-4911-8459-6324b12c7766")
		)
		(fp_line
			(start 3.89 5.59)
			(end 3.89 0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b761a04f-5b2e-4028-a365-194b590c6b31")
		)
		(fp_line
			(start 3.89 0.59)
			(end 5.11 0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "06d7c527-ffd4-4e9b-ab1c-03f4cca027d6")
		)
		(fp_line
			(start 3.89 -1.61)
			(end 3.89 0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8f07bd15-f5bd-40d6-9cb4-2fa26c0e7f38")
		)
		(fp_line
			(start 2.82 5.01)
			(end 2.82 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "df7439e0-7a9a-48db-8e74-5d1de2276da9")
		)
		(fp_line
			(start 2.82 1.59)
			(end 2.5 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "53626874-470e-4960-b850-82e2cef1100f")
		)
		(fp_line
			(start 2.5 5.09)
			(end 2.82 5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9a9054d9-3338-4647-acea-6a14118b3d72")
		)
		(fp_line
			(start 2.5 1.59)
			(end 2.18 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1f40081a-743b-45f7-94d4-c901985d0656")
		)
		(fp_line
			(start 2.18 5.01)
			(end 2.5 5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c473dae2-3f74-4f4a-bd03-007c56cdfbb4")
		)
		(fp_line
			(start 2.18 1.59)
			(end 2.18 5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "21fd93b8-09ce-4a8e-a6c8-d5b16ce67236")
		)
		(fp_line
			(start 1.17 0.59)
			(end 1.33 0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "aa2dfc5a-2904-4be6-9865-fec001dc5c48")
		)
		(fp_line
			(start 0.32 5.01)
			(end 0.32 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0c2a9d1a-1684-432b-b709-966d3bc4b5ef")
		)
		(fp_line
			(start 0.32 1.59)
			(end 0 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cd9d2268-761b-41d7-9567-255336f5e3e0")
		)
		(fp_line
			(start 0.3 -2.1)
			(end 0 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b2c7a022-e7dd-4422-a158-dfa7870e39bd")
		)
		(fp_line
			(start 0 5.09)
			(end 0.32 5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b889bc57-811b-4747-a65e-6a1b5ffef6d4")
		)
		(fp_line
			(start 0 1.59)
			(end -0.32 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b5786004-2398-48ef-a882-6abb4dd6452e")
		)
		(fp_line
			(start 0 -1.5)
			(end -0.3 -2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "dbe546a7-e6c9-40e5-a976-8c5bb0f5957f")
		)
		(fp_line
			(start -0.3 -2.1)
			(end 0.3 -2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "913e24ab-d006-4d1a-b9cf-fa84f8d30509")
		)
		(fp_line
			(start -0.32 5.01)
			(end 0 5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "929c6728-1ec8-4203-8318-9d15cf57b737")
		)
		(fp_line
			(start -0.32 1.59)
			(end -0.32 5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4443365b-4887-4257-98a0-a053e85630df")
		)
		(fp_line
			(start -1.39 5.59)
			(end -1.39 0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4f09e547-fd52-4c5c-bc63-11541274cf9e")
		)
		(fp_line
			(start -1.39 1.59)
			(end 3.89 1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bc14f72b-7aa4-4847-a523-e24b21e8ae72")
		)
		(fp_line
			(start -1.39 0.59)
			(end -1.39 -1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "08b1b1ee-7102-431a-82cc-073c6afc9d08")
		)
		(fp_line
			(start -1.39 0.59)
			(end -2.61 0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4fb9e48e-4c95-4ab3-823c-eb6c50f285d4")
		)
		(fp_line
			(start -1.39 -1.61)
			(end -2.61 -1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6978507f-5302-4dea-af51-9635d5d1ffaa")
		)
		(fp_line
			(start -2.61 6.81)
			(end 5.11 6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f65aada2-2cd2-4c15-a62f-0ed75073c451")
		)
		(fp_line
			(start -2.61 5.59)
			(end -1.39 5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c014a323-98f8-44e0-a5bf-c1dcfac8c1e4")
		)
		(fp_line
			(start -2.61 -1.61)
			(end -2.61 6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "669f2ba9-7537-46d9-8a47-a2ff7063e7f0")
		)
		(fp_line
			(start 5.5 7.2)
			(end -3 7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "409fc09e-c67b-4674-8d42-8970429c3f5f")
		)
		(fp_line
			(start 5.5 -2)
			(end 5.5 7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "62dc442c-b635-42b8-969e-26ee9e207fd9")
		)
		(fp_line
			(start -3 7.2)
			(end -3 -2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d6b38699-c4d5-4adc-869a-259590e1133f")
		)
		(fp_line
			(start -3 -2)
			(end 5.5 -2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "017d38dd-4a12-46f7-9464-18dd272471a9")
		)
		(fp_line
			(start 5 6.7)
			(end 5 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "44a5670b-a4e2-411a-b7af-bdfa6b7277d8")
		)
		(fp_line
			(start 5 -1.5)
			(end 4 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "de644d36-b793-43a4-94a8-a3641a583dd2")
		)
		(fp_line
			(start 4 0.7)
			(end -1.5 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c6a6435e-002b-4943-ac08-9cce9a2ae9f6")
		)
		(fp_line
			(start 4 -1.5)
			(end 4 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "35415799-b164-4b88-86c9-09e6e9038258")
		)
		(fp_line
			(start 0 1.407107)
			(end 0.5 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "18c423b4-4855-41e5-b14d-f68730e6cafd")
		)
		(fp_line
			(start -0.5 0.7)
			(end 0 1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "53dbf1d8-c5c5-44d2-b0c6-55f6a4652825")
		)
		(fp_line
			(start -1.5 0.7)
			(end -1.5 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7ea0e45f-7267-4afc-ba73-b72db84fb58a")
		)
		(fp_line
			(start -1.5 -1.5)
			(end -2.5 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6fff732b-3edf-4432-a765-7e32d2668d4c")
		)
		(fp_line
			(start -2.5 6.7)
			(end 5 6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6bafe221-0397-49e0-9a90-5882a6be59a9")
		)
		(fp_line
			(start -2.5 -1.5)
			(end -2.5 6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1d39516a-b82a-4a22-8483-f721eaf56d0f")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.6 0)
			(layer "B.Fab")
			(uuid "39583159-e387-43a7-a07b-e4d0cd7e5fa1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.2 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 30 "Net-(Battery1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "a2bc8dcc-37e0-468f-8182-79cc8cfc58d7")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 2.2 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+BATT")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "23e693dc-a1f4-4a2a-b25c-88d5c4058430")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S2B-EH_1x02_P2.50mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "B.Cu")
		(uuid "bdc129f0-b298-4fb7-a8a8-32a8f9742dd4")
		(at 193.334 131.318)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, diameter=5mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm diameter 5mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 1.25 3.75 0)
			(layer "B.SilkS")
			(uuid "1fc8dbd9-edbf-4a99-92a3-adb9e75a5cbd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "C_Polarized"
			(at 1.25 -3.75 0)
			(layer "B.Fab")
			(uuid "0bb67757-0644-49dc-be53-d5047c4c3397")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "07ebc7ec-6b00-4a20-86ee-8ae34fd0169d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "b1aa1f60-ec7d-4e39-b209-836a24d1d1af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/4ed24efe-cb72-4927-b8c3-11a395c26537")
		(sheetname "/")
		(sheetfile "espsnake.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.554775 1.475)
			(end -1.054775 1.475)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "dd33e6ac-e753-4107-818b-e73f8b6fa9ba")
		)
		(fp_line
			(start -1.304775 1.725)
			(end -1.304775 1.225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7d1de74e-d937-4173-bf57-386ef9f02b6f")
		)
		(fp_line
			(start 1.25 2.58)
			(end 1.25 -2.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "19bdc813-2bd2-49c5-8ff6-72ad5772ca64")
		)
		(fp_line
			(start 1.29 2.58)
			(end 1.29 -2.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a3c403b3-08c4-4250-8eda-f39be8216e5c")
		)
		(fp_line
			(start 1.33 2.579)
			(end 1.33 -2.579)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2806f893-f6c4-469f-97ed-6273adb6bd8e")
		)
		(fp_line
			(start 1.37 2.577)
			(end 1.37 -2.577)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1b9a1cf0-de61-418b-ac95-0f35c57d9d26")
		)
		(fp_line
			(start 1.41 2.575)
			(end 1.41 -2.575)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d11dbfcb-1eba-4c4f-8fc8-9ac0c96dde75")
		)
		(fp_line
			(start 1.45 2.572)
			(end 1.45 -2.572)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bbb739e9-96b3-48e5-8378-240598fc1ea9")
		)
		(fp_line
			(start 1.49 -1.04)
			(end 1.49 -2.569)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4e5a429f-05d8-405d-ac17-397f39eab15b")
		)
		(fp_line
			(start 1.49 2.569)
			(end 1.49 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8bfadb04-bf15-4a27-b30c-41a19d2a9e01")
		)
		(fp_line
			(start 1.53 -1.04)
			(end 1.53 -2.565)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "87895dd5-d62e-48b4-9b67-b049a100b765")
		)
		(fp_line
			(start 1.53 2.565)
			(end 1.53 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9ee93bb6-59b8-4891-8bcc-ab052634cc68")
		)
		(fp_line
			(start 1.57 -1.04)
			(end 1.57 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9bbfaac2-1ea5-4d23-b8f4-53302cc10b03")
		)
		(fp_line
			(start 1.57 2.56)
			(end 1.57 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "47ade251-2764-42e2-b483-5d5baa9afbdf")
		)
		(fp_line
			(start 1.61 -1.04)
			(end 1.61 -2.555)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "edb12e3a-e663-44cb-969c-cf84a6c35fae")
		)
		(fp_line
			(start 1.61 2.555)
			(end 1.61 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "803fec62-3e73-4a85-9170-6e36ff128a54")
		)
		(fp_line
			(start 1.65 -1.04)
			(end 1.65 -2.549)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6b652272-2b5c-4bc8-85db-8d6e1bb19351")
		)
		(fp_line
			(start 1.65 2.549)
			(end 1.65 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "54ba4572-cdef-47ce-bc93-daded1299036")
		)
		(fp_line
			(start 1.69 -1.04)
			(end 1.69 -2.543)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b12fa64d-9a45-46fa-906f-0c98748927de")
		)
		(fp_line
			(start 1.69 2.543)
			(end 1.69 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ea640663-b70e-4e2c-be06-a5900ff4ce5f")
		)
		(fp_line
			(start 1.73 -1.04)
			(end 1.73 -2.536)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8dcfa511-7594-4ec6-bc03-e7f0460905df")
		)
		(fp_line
			(start 1.73 2.536)
			(end 1.73 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fe9b2d68-29c3-40fd-b5dc-f0f896600faa")
		)
		(fp_line
			(start 1.77 -1.04)
			(end 1.77 -2.528)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9a811cb2-ae88-46e8-bd91-798d6e139c29")
		)
		(fp_line
			(start 1.77 2.528)
			(end 1.77 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8a03f9f6-d0b7-4b02-ba71-892a43c717e3")
		)
		(fp_line
			(start 1.81 -1.04)
			(end 1.81 -2.519)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3d3173ec-81aa-4963-a7c4-4e7fa40a7636")
		)
		(fp_line
			(start 1.81 2.519)
			(end 1.81 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "00ea1eb5-c33c-4339-aaad-d53e96fa602b")
		)
		(fp_line
			(start 1.85 -1.04)
			(end 1.85 -2.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3c667e45-6f40-4bf3-a3cf-502d0e868816")
		)
		(fp_line
			(start 1.85 2.51)
			(end 1.85 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "021ac3c2-7ed3-4f64-9776-2a0d32b74c7c")
		)
		(fp_line
			(start 1.89 -1.04)
			(end 1.89 -2.501)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "70a253fd-6e49-4295-854e-c010bb799667")
		)
		(fp_line
			(start 1.89 2.501)
			(end 1.89 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "67d292a5-aef7-4b12-9697-06f40aa47302")
		)
		(fp_line
			(start 1.93 -1.04)
			(end 1.93 -2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9f649922-3c57-4c8d-b883-748decdeedd1")
		)
		(fp_line
			(start 1.93 2.49)
			(end 1.93 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b19eaeb5-aabb-46f6-9843-37f99593b6ea")
		)
		(fp_line
			(start 1.97 -1.04)
			(end 1.97 -2.479)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "329d060e-30be-41b9-8b2e-809b0e2e690b")
		)
		(fp_line
			(start 1.97 2.479)
			(end 1.97 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5aab873d-8791-4fe1-bf2a-8c265522b71e")
		)
		(fp_line
			(start 2.01 -1.04)
			(end 2.01 -2.467)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "62374a16-35af-48c7-80fa-673279061dbd")
		)
		(fp_line
			(start 2.01 2.467)
			(end 2.01 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a2e2aab0-ba15-40f0-92db-de36170d3c2b")
		)
		(fp_line
			(start 2.05 -1.04)
			(end 2.05 -2.455)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c5b71484-5542-4bce-b1b7-0d2c0b1c6b60")
		)
		(fp_line
			(start 2.05 2.455)
			(end 2.05 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5a7dc198-709f-4300-874d-fd8caf19b843")
		)
		(fp_line
			(start 2.09 -1.04)
			(end 2.09 -2.442)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "022d9601-6476-41dd-ba54-865a8f7cfecc")
		)
		(fp_line
			(start 2.09 2.442)
			(end 2.09 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2a2239ed-e7b3-4c44-b8fc-a2b4f6da500a")
		)
		(fp_line
			(start 2.13 -1.04)
			(end 2.13 -2.428)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "762a7d4e-566c-45fc-8d24-31305ae40dec")
		)
		(fp_line
			(start 2.13 2.428)
			(end 2.13 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5176459c-8ced-494f-9562-65675dd3d0c3")
		)
		(fp_line
			(start 2.17 -1.04)
			(end 2.17 -2.413)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "425f8053-0d7a-4f19-a6bc-319395fabf60")
		)
		(fp_line
			(start 2.17 2.413)
			(end 2.17 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "00b2446c-f365-4e07-a09d-af23d995aee3")
		)
		(fp_line
			(start 2.21 -1.04)
			(end 2.21 -2.398)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "82d1fcf5-e714-4c91-990a-9cc1c2b0b67e")
		)
		(fp_line
			(start 2.21 2.398)
			(end 2.21 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d60bf140-0a1d-4d37-96e2-356c67a051a0")
		)
		(fp_line
			(start 2.25 -1.04)
			(end 2.25 -2.382)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9e5b0396-94cf-4085-be71-13e824cf4513")
		)
		(fp_line
			(start 2.25 2.382)
			(end 2.25 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6c9abefe-eb05-43aa-a0cd-487eec3f8164")
		)
		(fp_line
			(start 2.29 -1.04)
			(end 2.29 -2.365)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1bd7e387-9ea3-40a7-9cbc-b8bbfa89cd3f")
		)
		(fp_line
			(start 2.29 2.365)
			(end 2.29 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5ba735fb-e5f7-452f-9d70-443cf512235f")
		)
		(fp_line
			(start 2.33 -1.04)
			(end 2.33 -2.347)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "28bdd568-9efb-45da-8f1b-5afa1197a3b3")
		)
		(fp_line
			(start 2.33 2.347)
			(end 2.33 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9e03bf8e-fb3e-417c-8ab7-275f75e82706")
		)
		(fp_line
			(start 2.37 -1.04)
			(end 2.37 -2.329)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f4eb8345-9b17-48b1-b9e0-b3a126d31fc4")
		)
		(fp_line
			(start 2.37 2.329)
			(end 2.37 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "17698987-ba65-4a15-81b9-2b171a07d5b3")
		)
		(fp_line
			(start 2.41 -1.04)
			(end 2.41 -2.309)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4c994157-1bbb-4b4e-934c-63ddb815045c")
		)
		(fp_line
			(start 2.41 2.309)
			(end 2.41 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cdfdd811-e7f2-48fa-9300-653c1df9f239")
		)
		(fp_line
			(start 2.45 -1.04)
			(end 2.45 -2.289)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ce2742ca-d628-41a1-b32f-db76e0910f10")
		)
		(fp_line
			(start 2.45 2.289)
			(end 2.45 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "08ca3d2e-500f-47cb-aed0-96e2ab7e2ebf")
		)
		(fp_line
			(start 2.49 -1.04)
			(end 2.49 -2.268)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9df34a14-2101-432d-b06b-ff10332a1c24")
		)
		(fp_line
			(start 2.49 2.268)
			(end 2.49 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c5242152-91b8-4eb2-83ed-aa73d8b1a60c")
		)
		(fp_line
			(start 2.53 -1.04)
			(end 2.53 -2.246)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1a5850e6-6bd6-463b-b679-fced4b55a3b9")
		)
		(fp_line
			(start 2.53 2.246)
			(end 2.53 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "59aec842-0e34-4222-b2ba-f0ba23bba600")
		)
		(fp_line
			(start 2.57 -1.04)
			(end 2.57 -2.223)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2da06f7f-2856-4081-b555-40a14579e7dc")
		)
		(fp_line
			(start 2.57 2.223)
			(end 2.57 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b3deacdc-18f0-418f-8f2a-29f7685f2f26")
		)
		(fp_line
			(start 2.61 -1.04)
			(end 2.61 -2.199)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1f190636-4ec2-4549-829f-b563a471f2ec")
		)
		(fp_line
			(start 2.61 2.199)
			(end 2.61 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "92be2aa2-a066-437c-8646-31ff53581905")
		)
		(fp_line
			(start 2.65 -1.04)
			(end 2.65 -2.175)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d1beb341-80da-422c-8008-7c4f7b7d8f59")
		)
		(fp_line
			(start 2.65 2.175)
			(end 2.65 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b49e6d19-cf2c-4ab8-8535-1fa6d7e911f0")
		)
		(fp_line
			(start 2.69 -1.04)
			(end 2.69 -2.149)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "22e34a1d-200d-4387-922e-4bfba74ce1a8")
		)
		(fp_line
			(start 2.69 2.149)
			(end 2.69 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "48815c6e-1430-44a2-b426-b701dd8c3675")
		)
		(fp_line
			(start 2.73 -1.04)
			(end 2.73 -2.122)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "65cd1765-35b1-42b8-898a-f550739a0839")
		)
		(fp_line
			(start 2.73 2.122)
			(end 2.73 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "04544184-faac-42a7-b510-69b852ceefae")
		)
		(fp_line
			(start 2.77 -1.04)
			(end 2.77 -2.094)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c1434707-3697-451a-b462-0781f0fe9b9b")
		)
		(fp_line
			(start 2.77 2.094)
			(end 2.77 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2136d8a3-268f-45c4-8eaf-cb54f26d373d")
		)
		(fp_line
			(start 2.81 -1.04)
			(end 2.81 -2.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "628b7512-e66d-491e-9efa-0d33321bbca3")
		)
		(fp_line
			(start 2.81 2.065)
			(end 2.81 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c21ae530-2552-430a-a143-fcea945a9060")
		)
		(fp_line
			(start 2.85 -1.04)
			(end 2.85 -2.035)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fb193de4-4a94-45a8-87c4-01efc4fe6703")
		)
		(fp_line
			(start 2.85 2.035)
			(end 2.85 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2fa0cc9d-50d5-475b-b11e-78dd8ab29947")
		)
		(fp_line
			(start 2.89 -1.04)
			(end 2.89 -2.003)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2a13d078-f99d-4c1d-b662-10d958dad8da")
		)
		(fp_line
			(start 2.89 2.003)
			(end 2.89 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "18bd67e0-4940-42cd-985b-e59df56197c1")
		)
		(fp_line
			(start 2.93 -1.04)
			(end 2.93 -1.97)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "42772ced-18a3-4d0a-ba54-3b7f64ebaf00")
		)
		(fp_line
			(start 2.93 1.97)
			(end 2.93 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6b3dee47-5f20-40de-9a3f-22ba2b313860")
		)
		(fp_line
			(start 2.97 -1.04)
			(end 2.97 -1.936)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "325f542b-6896-4596-bfeb-6c635e6ebbd3")
		)
		(fp_line
			(start 2.97 1.936)
			(end 2.97 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bba72604-f229-45fe-92ba-5a476338f1a8")
		)
		(fp_line
			(start 3.01 -1.04)
			(end 3.01 -1.901)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "39548524-e453-4b7b-8909-901faa5ea1e1")
		)
		(fp_line
			(start 3.01 1.901)
			(end 3.01 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3b891ae0-1049-4e44-9c4e-7a6a5d4c457f")
		)
		(fp_line
			(start 3.05 -1.04)
			(end 3.05 -1.864)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bb4226bf-124e-4336-b7dd-1783a35e5917")
		)
		(fp_line
			(start 3.05 1.864)
			(end 3.05 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f9c7bcbe-920e-44a4-86d0-3377fdc9227d")
		)
		(fp_line
			(start 3.09 -1.04)
			(end 3.09 -1.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b74d0d78-6a1e-4c99-8816-a1790dd1a0ea")
		)
		(fp_line
			(start 3.09 1.825)
			(end 3.09 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c16e6a8a-5fac-420f-8543-1ddea87b750b")
		)
		(fp_line
			(start 3.13 -1.04)
			(end 3.13 -1.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "27824759-4727-46de-ada2-01406e14bc1a")
		)
		(fp_line
			(start 3.13 1.785)
			(end 3.13 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d6654dab-6466-4ef1-9739-f00afc98bfb2")
		)
		(fp_line
			(start 3.17 -1.04)
			(end 3.17 -1.743)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6dc0a8b0-2308-4c2b-8d64-b00e6a84e677")
		)
		(fp_line
			(start 3.17 1.743)
			(end 3.17 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "61e3f335-a044-4e15-84f1-d3246a40baa1")
		)
		(fp_line
			(start 3.21 -1.04)
			(end 3.21 -1.699)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f85911a9-6ab2-4383-a408-c397e462bfd0")
		)
		(fp_line
			(start 3.21 1.699)
			(end 3.21 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d7420025-4095-4fa0-b802-a9d194cef7ab")
		)
		(fp_line
			(start 3.25 -1.04)
			(end 3.25 -1.652)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3b51d173-2e79-40ef-a049-1e9d6b3e6fb4")
		)
		(fp_line
			(start 3.25 1.652)
			(end 3.25 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1a7793ec-9c49-40aa-9365-460815d84d06")
		)
		(fp_line
			(start 3.29 -1.04)
			(end 3.29 -1.604)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d6f39657-0840-4859-9808-53c7f945aab0")
		)
		(fp_line
			(start 3.29 1.604)
			(end 3.29 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5757a15a-8709-46c3-9938-afd5e5db35c1")
		)
		(fp_line
			(start 3.33 -1.04)
			(end 3.33 -1.553)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "559969ad-9062-480b-8c90-19babcf57625")
		)
		(fp_line
			(start 3.33 1.553)
			(end 3.33 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e63e435c-0c93-4d8e-bffb-aca8e30b4ab1")
		)
		(fp_line
			(start 3.37 -1.04)
			(end 3.37 -1.499)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0e122300-2066-4bcf-ba26-ed3cf37a84a3")
		)
		(fp_line
			(start 3.37 1.499)
			(end 3.37 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d7f31ced-1087-42d5-b528-64a248b45c81")
		)
		(fp_line
			(start 3.41 -1.04)
			(end 3.41 -1.443)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ec953b5d-a747-4962-bf4e-8b9780166285")
		)
		(fp_line
			(start 3.41 1.443)
			(end 3.41 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "24d7b677-871e-4b91-8fd5-ed47de7ccd11")
		)
		(fp_line
			(start 3.45 -1.04)
			(end 3.45 -1.383)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a8e3daa9-5f2c-4f74-aee6-e6b7e444c537")
		)
		(fp_line
			(start 3.45 1.383)
			(end 3.45 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "63d56369-9595-44d7-a536-a9729147e602")
		)
		(fp_line
			(start 3.49 -1.04)
			(end 3.49 -1.319)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "55df146c-0261-4ada-bb82-797e8a4338c8")
		)
		(fp_line
			(start 3.49 1.319)
			(end 3.49 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "242eb15c-9250-4dce-9d2c-b6bc2669c607")
		)
		(fp_line
			(start 3.53 -1.04)
			(end 3.53 -1.251)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4016ea5d-dfa1-4a1e-94cf-27ac54b6a450")
		)
		(fp_line
			(start 3.53 1.251)
			(end 3.53 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a233c55d-6327-4f0e-ab8f-80aacd9e52f7")
		)
		(fp_line
			(start 3.57 1.177)
			(end 3.57 -1.177)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "dd7ce27d-881e-47a5-8258-3e2dfae1a2be")
		)
		(fp_line
			(start 3.61 1.098)
			(end 3.61 -1.098)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "71c81055-a04b-4b0f-99c6-7806cdd1c12a")
		)
		(fp_line
			(start 3.65 1.011)
			(end 3.65 -1.011)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f2ba9748-8872-4380-9a1f-50461d2de732")
		)
		(fp_line
			(start 3.69 0.914)
			(end 3.69 -0.914)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "929eaceb-5d89-4582-a10b-55bf0d3b364c")
		)
		(fp_line
			(start 3.73 0.805)
			(end 3.73 -0.805)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f76bf60d-8a25-44ae-a2a5-7fd66283bb5a")
		)
		(fp_line
			(start 3.77 0.677)
			(end 3.77 -0.677)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "62c98b17-f67b-44db-bc53-36ef68d653a8")
		)
		(fp_line
			(start 3.81 0.517)
			(end 3.81 -0.517)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "aeda11f3-e80d-4c27-abcd-9845102b5b22")
		)
		(fp_line
			(start 3.85 0.283)
			(end 3.85 -0.283)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bf13f867-8e71-40c3-a738-a13124c9e87e")
		)
		(fp_circle
			(center 1.25 0)
			(end 3.87 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "17f16c8c-21ca-4e0d-897a-931499e88684")
		)
		(fp_circle
			(center 1.25 0)
			(end 4 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "d15826ca-849f-4ae6-9eb9-18d858f6dffb")
		)
		(fp_line
			(start -0.883605 1.0875)
			(end -0.383605 1.0875)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a0cb8b5e-2f6b-456e-aa00-ffe05e03ec29")
		)
		(fp_line
			(start -0.633605 1.3375)
			(end -0.633605 0.8375)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c498d350-fba4-4d41-8c65-7e4b7ba3f94f")
		)
		(fp_circle
			(center 1.25 0)
			(end 3.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "b5788db2-0554-44c8-be48-1d089213739c")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "B.Fab")
			(uuid "ded3fac2-7d17-4c3e-877b-369fcb2aae88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.3 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 5 "+BATT")
			(pintype "passive")
			(uuid "11e053f8-b0ca-4055-b09b-e6434e50f7d5")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 2.3 2.3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
			(uuid "4ab304ff-fedd-47ae-b989-95f0fc561a64")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 182.118 52.07)
		(end 224.79 146.558)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "Margin")
		(uuid "07775fe9-ac4b-4d58-a2c0-b084378c6e3d")
	)
	(segment
		(start 191.014 120.148)
		(end 183.388 112.522)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "2ed8d125-9826-4f84-8580-3981feebfaea")
	)
	(segment
		(start 183.388 112.522)
		(end 183.388 100.33)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "32f96c79-3dca-4c95-aca1-9a61d112ac73")
	)
	(segment
		(start 209.296 74.676)
		(end 209.296 76.708)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "45d9c368-f16b-4886-afa9-dc1030c88702")
	)
	(segment
		(start 183.388 100.33)
		(end 195.072 88.646)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "55269504-fd8a-4a51-8a2e-11c45a2457a8")
	)
	(segment
		(start 208.026 73.406)
		(end 209.296 74.676)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "62309ffd-0c33-4429-ae50-afcf8ee45d1e")
	)
	(segment
		(start 209.296 76.708)
		(end 207.01 78.994)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "8c452a60-46f1-439c-afe9-10fb8f6ba7e9")
	)
	(segment
		(start 191.014 122.539)
		(end 191.014 120.148)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "c4b88f6e-9d99-4dc9-8d06-361146d7e2da")
	)
	(segment
		(start 207.01 78.994)
		(end 207.01 87.15)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "e4962c5d-c1b2-4d23-9f70-53e35d209c88")
	)
	(segment
		(start 197.866 73.406)
		(end 208.026 73.406)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "ece697f9-3c23-477a-a304-7cc9c4bffbcd")
	)
	(segment
		(start 195.072 76.2)
		(end 197.866 73.406)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "f52a3d10-fa8e-4e6c-9568-0311b0593dd4")
	)
	(segment
		(start 195.072 88.646)
		(end 195.072 76.2)
		(width 0.75)
		(layer "B.Cu")
		(net 1)
		(uuid "fe5362d4-186f-4746-8db2-e2193820bc1e")
	)
	(segment
		(start 211.836 130.176)
		(end 211.836 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "0a0b2a75-96d0-4bd1-b292-1a9c3fcd1461")
	)
	(segment
		(start 192.01 110.35)
		(end 196.95 105.41)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "0e963a6e-2348-429e-a97b-3dabc5d905e7")
	)
	(segment
		(start 216.854 139.479001)
		(end 216.854 139.884)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "24b77b2e-c622-40a0-8820-ca0a0018a963")
	)
	(segment
		(start 214.39 122.85)
		(end 209.45 127.79)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "3c6038e9-f814-41ee-96d0-55c3808e53f0")
	)
	(segment
		(start 209.45 127.79)
		(end 211.836 130.176)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "3d432efa-a935-474b-8133-df68c1e787d4")
	)
	(segment
		(start 195.834 138.15)
		(end 198.7 138.15)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "4f46923d-e380-4a74-97a8-106356ec84b6")
	)
	(segment
		(start 211.836 137.979)
		(end 210.566 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "504a2978-8193-48ed-99cc-be0cf3e2f9aa")
	)
	(segment
		(start 216.219 140.519)
		(end 216.854 139.884)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "5c91bdc2-4bab-4ecb-8155-502d15ef7729")
	)
	(segment
		(start 210.566 137.979)
		(end 207.529 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "60f59dce-f1a7-4d6c-bac6-4d09eff504bb")
	)
	(segment
		(start 214.379 140.519)
		(end 216.219 140.519)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "6a4c436f-ab7e-4811-9514-e3baecd7adbd")
	)
	(segment
		(start 214.39 110.35)
		(end 214.39 122.85)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "7c2654a6-5d8a-4b77-a630-78336a7e7d64")
	)
	(segment
		(start 196.95 127.79)
		(end 192.01 122.85)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "7e009736-fe39-4a88-9049-d0aca04f48be")
	)
	(segment
		(start 192.01 122.85)
		(end 192.01 110.35)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "7e97940b-3b18-4e47-bf49-05b21c2a49c0")
	)
	(segment
		(start 195.834 128.906)
		(end 196.95 127.79)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "84f48f34-a939-48af-8619-175404d427b6")
	)
	(segment
		(start 195.834 131.318)
		(end 195.834 128.906)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "92027c65-e139-4ce7-97e6-8fff32351afd")
	)
	(segment
		(start 210.566 138.176)
		(end 210.566 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "9c9517ce-6eb4-4d7a-8ca9-a37eab748a30")
	)
	(segment
		(start 207.529 137.979)
		(end 207.52 137.97)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "9d1aef4c-6639-4773-8eed-73492f376acc")
	)
	(segment
		(start 209.45 127.79)
		(end 196.95 127.79)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "a4ada04e-2bef-43fc-a017-90259d1c5c51")
	)
	(segment
		(start 196.95 105.41)
		(end 205.232 105.41)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "ab11a911-0c8a-4802-afda-3cec18604695")
	)
	(segment
		(start 209.45 105.41)
		(end 214.39 110.35)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "ab29f235-be28-4cb5-a502-0d0e133cf153")
	)
	(segment
		(start 184.909 135.677)
		(end 185.525 136.293)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "ae6435b4-b07e-4e2e-9478-463e95b0b588")
	)
	(segment
		(start 214.39 110.35)
		(end 214.39 110.222)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "ba6bf922-a889-4b23-88b7-5a2e823e4edb")
	)
	(segment
		(start 205.232 105.41)
		(end 209.45 105.41)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "c8fcb5ab-2371-4e56-9127-4a213269b54d")
	)
	(segment
		(start 184.909 135.636)
		(end 184.909 135.677)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "d572fd01-a79c-4f47-bb4f-d41df355669a")
	)
	(segment
		(start 198.7 138.15)
		(end 198.88 137.97)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "d6d1576d-9945-4a3c-b763-e4b9c641faf7")
	)
	(segment
		(start 215.353999 137.979)
		(end 216.854 139.479001)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "d8f8c60f-fc55-443f-a755-8c0e27e8aa22")
	)
	(segment
		(start 214.379 137.979)
		(end 211.836 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "dc0f0dec-26a1-4703-a6dc-abbe79e0a9f4")
	)
	(segment
		(start 185.525 136.293)
		(end 185.525 138.09)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "e9646cc9-0099-40ea-9a9d-8fe323097cc5")
	)
	(segment
		(start 214.379 137.979)
		(end 215.353999 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 2)
		(uuid "f8022823-1780-4fea-8c80-8ccee388b53e")
	)
	(via
		(at 184.909 135.636)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(net 2)
		(uuid "1fbc1de6-1231-427f-b4b1-6bba89d2b409")
	)
	(segment
		(start 205.232 114.554)
		(end 210.058 109.728)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "0092d37a-368c-42a7-b9a4-18d1a9a50aa4")
	)
	(segment
		(start 222.758 126.746)
		(end 211.534 137.97)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "0412f267-bbe0-413d-ab79-fce50846305a")
	)
	(segment
		(start 210.058 109.728)
		(end 210.058 103.124)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "12c6e4c6-6443-434c-a77c-e8c27f6a277b")
	)
	(segment
		(start 195.834 132.842)
		(end 193.294 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "137c419f-3512-43ff-8107-9f8dc43697ee")
	)
	(segment
		(start 207.52 135.612)
		(end 207.29 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "18a635f0-85f5-479d-a384-6993c4ff2d03")
	)
	(segment
		(start 198.88 137.97)
		(end 198.88 135.612)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "19164cd7-9e0a-4cbd-a344-e395e1fc4fa7")
	)
	(segment
		(start 198.88 141.77)
		(end 198.88 137.97)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "27ba2c5e-28d3-4067-a2ee-c19cc3aefd10")
	)
	(segment
		(start 191.659466 135.382)
		(end 185.163 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "29b8ae79-c6ad-4a15-89bd-ddb332414836")
	)
	(segment
		(start 185.163 135.382)
		(end 184.909 135.636)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "2cc4f572-1c06-4c58-9d69-df61d7bf8a36")
	)
	(segment
		(start 219.964 103.378)
		(end 219.964 121.666)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "374466e6-802c-4b43-b6d4-ea57ddfdf861")
	)
	(segment
		(start 198.88 135.612)
		(end 199.11 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "38e15435-ee93-4feb-a97f-3ed842c16abf")
	)
	(segment
		(start 211.328 101.854)
		(end 217.424 101.854)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "3cacb1c3-4a4f-418b-8b97-299e326626e1")
	)
	(segment
		(start 211.074 95.758)
		(end 221.488 95.758)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "41edc31b-3a69-4350-a7cf-5ff9d368597b")
	)
	(segment
		(start 207.52 141.77)
		(end 207.52 135.612)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "42100ec3-d3ac-4290-8f46-2d738b94fd44")
	)
	(segment
		(start 195.834 131.318)
		(end 195.834 132.842)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "4432b1e9-6e95-4967-aa51-6499b89540c2")
	)
	(segment
		(start 207.44 137.89)
		(end 207.52 137.97)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "4c281c7d-4ce0-47bf-bef9-434618a5d1ec")
	)
	(segment
		(start 220.98 103.378)
		(end 219.964 103.378)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "4ea0d59c-c5ca-4da9-b64e-539b75ebebe3")
	)
	(segment
		(start 200.45 137.89)
		(end 198.96 137.89)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "50e37b56-d50c-424d-bc09-093388a15427")
	)
	(segment
		(start 222.504 101.854)
		(end 220.98 103.378)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "5c577272-2bbf-4383-bb89-bac1c8bdf432")
	)
	(segment
		(start 219.964 121.666)
		(end 222.758 124.46)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "679b5187-7662-4656-84f0-7119da62c3b1")
	)
	(segment
		(start 195.834 129.794)
		(end 195.834 131.318)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "68be7946-ef54-4708-81dd-588d78799613")
	)
	(segment
		(start 195.072 129.032)
		(end 195.834 129.794)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "81328349-0d1f-4860-b6f6-6d1d3b1f6e30")
	)
	(segment
		(start 195.834 135.382)
		(end 191.659466 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "882df31c-ea20-4e13-ae29-bcfd9510042b")
	)
	(segment
		(start 188.474 122.539)
		(end 188.474 124.72)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "8d51a37f-2257-4fc0-acf8-27995d8e2d53")
	)
	(segment
		(start 221.488 95.758)
		(end 222.504 96.774)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "92f9942d-8274-4662-8f0c-dacfb99da82a")
	)
	(segment
		(start 218.948 103.378)
		(end 219.964 103.378)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "9552fb28-1f32-4a03-8e60-19cd9abaef12")
	)
	(segment
		(start 204.47 78.232)
		(end 204.47 87.15)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "a1cb7515-941d-4bf4-8859-a6acbf9d4c1d")
	)
	(segment
		(start 204.47 87.15)
		(end 204.47 89.154)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "a2215c7f-ed71-4e0a-ba28-72456b2c66ee")
	)
	(segment
		(start 192.786 129.032)
		(end 195.072 129.032)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "a3c8fb58-8218-47cd-92b5-91b5cd537024")
	)
	(segment
		(start 217.424 101.854)
		(end 218.948 103.378)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "a448b8d7-2c61-435a-b09b-0b383825f952")
	)
	(segment
		(start 222.758 124.46)
		(end 222.758 126.746)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "a4c4497f-3d09-4262-b62b-414b72bb4c05")
	)
	(segment
		(start 198.96 137.89)
		(end 198.88 137.97)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "a9d94441-ff9f-4505-ae0c-20a9ed00f128")
	)
	(segment
		(start 207.01 75.692)
		(end 204.47 78.232)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "b16bae69-8c79-4f21-810f-4b21db2c9d66")
	)
	(segment
		(start 210.058 103.124)
		(end 211.328 101.854)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "b59c89e6-4e5d-4382-aeaf-f6b4b7d0f540")
	)
	(segment
		(start 204.47 89.154)
		(end 211.074 95.758)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "b60b3cda-e960-44cb-bfc0-f9df848eedec")
	)
	(segment
		(start 205.95 137.89)
		(end 207.44 137.89)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "bd4e6e97-975b-46c6-9d77-eb4ea893d30e")
	)
	(segment
		(start 211.534 137.97)
		(end 207.52 137.97)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "bdccf239-b495-478b-8279-8b77c5a23577")
	)
	(segment
		(start 222.504 96.774)
		(end 222.504 101.854)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "cc2dd664-e34b-4fe2-a11f-7260cd220aec")
	)
	(segment
		(start 193.294 135.382)
		(end 191.659466 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "cf399a01-b2ce-4958-b7c2-9f95a64674c8")
	)
	(segment
		(start 188.474 124.72)
		(end 192.786 129.032)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "ed7199ea-5817-4258-922a-17b0a8bb4786")
	)
	(segment
		(start 199.11 135.382)
		(end 195.834 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 2)
		(uuid "ffa86beb-c5f3-4459-9129-df5961e65f93")
	)
	(segment
		(start 196.094 104.908)
		(end 196.094 106.569)
		(width 0.75)
		(layer "B.Cu")
		(net 3)
		(uuid "06c63ecc-16df-4f08-a0b2-18727c793c8b")
	)
	(segment
		(start 201.93 87.15)
		(end 201.93 89.154)
		(width 0.75)
		(layer "B.Cu")
		(net 3)
		(uuid "652c9626-5707-47ee-a987-542c674a7cd5")
	)
	(segment
		(start 193.802 97.282)
		(end 193.802 102.616)
		(width 0.75)
		(layer "B.Cu")
		(net 3)
		(uuid "a35194b2-7a24-428f-80e7-e3eae5bd23d3")
	)
	(segment
		(start 201.93 89.154)
		(end 193.802 97.282)
		(width 0.75)
		(layer "B.Cu")
		(net 3)
		(uuid "d2c1e607-916b-4666-9573-994b30c51e4d")
	)
	(segment
		(start 193.802 102.616)
		(end 196.094 104.908)
		(width 0.75)
		(layer "B.Cu")
		(net 3)
		(uuid "ef0034c3-8672-4c5d-9096-da8ddc42a2d0")
	)
	(segment
		(start 199.39 87.15)
		(end 199.39 89.154)
		(width 0.75)
		(layer "B.Cu")
		(net 4)
		(uuid "0397ed76-a401-41af-b5d2-4c9cea6d7b9f")
	)
	(segment
		(start 193.294 104.394)
		(end 193.294 106.309)
		(width 0.75)
		(layer "B.Cu")
		(net 4)
		(uuid "0f0ce7dd-4b94-4a48-a405-535a98c20837")
	)
	(segment
		(start 192.024 103.124)
		(end 193.294 104.394)
		(width 0.75)
		(layer "B.Cu")
		(net 4)
		(uuid "58f01969-ea62-4848-a373-b20f0532e5d6")
	)
	(segment
		(start 193.294 106.309)
		(end 193.554 106.569)
		(width 0.75)
		(layer "B.Cu")
		(net 4)
		(uuid "63671c82-107f-49ea-a287-4b9fb9e7ce08")
	)
	(segment
		(start 199.39 89.154)
		(end 192.024 96.52)
		(width 0.75)
		(layer "B.Cu")
		(net 4)
		(uuid "db380c9c-211b-4261-ad87-e5a36c7d4644")
	)
	(segment
		(start 192.024 96.52)
		(end 192.024 103.124)
		(width 0.75)
		(layer "B.Cu")
		(net 4)
		(uuid "e500c794-8ce7-4c2d-a137-f316b127e8af")
	)
	(segment
		(start 186.944 135.128)
		(end 191.427 135.128)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "360f9bbb-4337-48f2-939a-fb03ed7639b0")
	)
	(segment
		(start 202.679 139.7)
		(end 195.113222 139.7)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "46329512-cedf-4761-95c4-b65a07ff3daa")
	)
	(segment
		(start 219.329 141.789)
		(end 215.576 145.542)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "514d768a-a228-4d29-9b79-bd4ea507b4b1")
	)
	(segment
		(start 185.948 134.132)
		(end 186.944 135.128)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "57aea908-1603-41b9-864d-15f063e21c8f")
	)
	(segment
		(start 195.113222 139.7)
		(end 193.6 138.186778)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "5f35c8a7-7894-474d-be4a-dca58b936bce")
	)
	(segment
		(start 215.576 145.542)
		(end 208.521 145.542)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "61b4ea6b-9a3d-492e-bd07-abc902717715")
	)
	(segment
		(start 208.521 145.542)
		(end 202.679 139.7)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "797ae2e4-bc22-4cb2-b092-8d446d8c497c")
	)
	(segment
		(start 193.6 138.186778)
		(end 193.6 138.176)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "8029e1e5-ea04-4f00-a395-ac958ad2dd96")
	)
	(segment
		(start 185.948 133.0885)
		(end 185.948 134.132)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "b59aa39c-59d1-4cf2-bcbd-9b0a13e8d2c9")
	)
	(segment
		(start 191.427 135.128)
		(end 193.6 137.301)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "b5c90285-af64-4ca8-b1a5-9e68c66ad276")
	)
	(segment
		(start 193.6 137.301)
		(end 193.6 138.176)
		(width 0.75)
		(layer "F.Cu")
		(net 5)
		(uuid "b96abc57-6b64-49bc-a3e0-567232ec17ef")
	)
	(segment
		(start 185.948 132.06)
		(end 187.198 130.81)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "277cb679-c38d-40c9-9b65-e95bfa995bbf")
	)
	(segment
		(start 185.934 124.974)
		(end 192.278 131.318)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "5bf56104-e10a-48a1-a168-8e0d4bbdaff0")
	)
	(segment
		(start 192.278 131.318)
		(end 193.334 131.318)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "601b91e5-73b2-4882-a7dd-e1c3979dd775")
	)
	(segment
		(start 187.198 130.81)
		(end 192.826 130.81)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "6fd06d7f-30da-47e3-98ec-3227f3b271c4")
	)
	(segment
		(start 185.934 122.539)
		(end 185.934 124.974)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "c14b95c6-ed5f-4ec3-b807-46e13e7a5788")
	)
	(segment
		(start 185.948 133.0885)
		(end 185.948 132.06)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "dfe7c804-efcc-4e21-97fb-7fd2b2a8a6a9")
	)
	(segment
		(start 192.826 130.81)
		(end 193.334 131.318)
		(width 0.75)
		(layer "B.Cu")
		(net 5)
		(uuid "f972f250-316d-4b11-b990-d44e7fb72c11")
	)
	(segment
		(start 192.024 137.16)
		(end 191.008 136.144)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "386d4db6-c5f5-46fb-ba70-2258ded13971")
	)
	(segment
		(start 188.595 136.144)
		(end 186.7 138.039)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "5c2d57a3-bb80-4baf-9847-c1a95097c937")
	)
	(segment
		(start 191.008 136.144)
		(end 188.595 136.144)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "6ae03ebd-1270-4900-8016-4e723f4f4bc0")
	)
	(segment
		(start 192.024 138.8825)
		(end 192.024 137.16)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "8683dbcb-1e7f-4c97-adf6-a5419087d541")
	)
	(segment
		(start 186.7 138.039)
		(end 186.7 138.09)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "d9e7c79b-1e64-4348-ab97-11d6ddbd16ec")
	)
	(segment
		(start 193.4155 140.274)
		(end 192.024 138.8825)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "ebd61a7e-c4fb-4acf-aa45-3748a8bd50c9")
	)
	(segment
		(start 193.4155 142.174)
		(end 190.3015 145.288)
		(width 0.5)
		(layer "F.Cu")
		(net 8)
		(uuid "71106570-61f0-47e7-99e9-0b912e0a341b")
	)
	(segment
		(start 190.3015 145.288)
		(end 187.579 145.288)
		(width 0.5)
		(layer "F.Cu")
		(net 8)
		(uuid "a87296dd-71c7-448b-8a10-d61f65a6134f")
	)
	(segment
		(start 187.579 145.288)
		(end 186.7 144.409)
		(width 0.5)
		(layer "F.Cu")
		(net 8)
		(uuid "d3f40154-a2bd-4a7e-9758-e9b17fc19c3c")
	)
	(segment
		(start 186.7 144.409)
		(end 186.7 143.85)
		(width 0.5)
		(layer "F.Cu")
		(net 8)
		(uuid "ed3d21e8-d6c1-4d41-8acd-1efc4fdeb4d7")
	)
	(segment
		(start 209.45 135.41)
		(end 209.45 132.942)
		(width 0.75)
		(layer "F.Cu")
		(net 10)
		(uuid "15fe1d07-810a-41c4-b8aa-4c6191be636e")
	)
	(segment
		(start 196.95 135.41)
		(end 209.45 135.41)
		(width 0.75)
		(layer "F.Cu")
		(net 10)
		(uuid "88a1d5f6-5334-4eaa-8d9c-0e2315525b83")
	)
	(segment
		(start 209.45 132.942)
		(end 209.804 132.588)
		(width 0.75)
		(layer "F.Cu")
		(net 10)
		(uuid "e962550a-ac44-4d53-9e13-a60b28e95984")
	)
	(via
		(at 209.804 132.588)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(free yes)
		(net 10)
		(uuid "bc847e9b-70d6-44be-bef6-0c26085d41ee")
	)
	(segment
		(start 196.094 122.539)
		(end 196.094 124.974)
		(width 0.75)
		(layer "B.Cu")
		(net 10)
		(uuid "3b034617-e538-41c9-b579-6bcc25147fc3")
	)
	(segment
		(start 196.094 117.85)
		(end 197.612 116.332)
		(width 0.75)
		(layer "B.Cu")
		(net 10)
		(uuid "5e75660b-a650-4cac-aa5d-7b067caffa1d")
	)
	(segment
		(start 196.094 122.539)
		(end 196.094 117.85)
		(width 0.75)
		(layer "B.Cu")
		(net 10)
		(uuid "a1fe3a07-23fe-4932-91a4-0b495d00a7e8")
	)
	(segment
		(start 196.094 124.974)
		(end 203.708 132.588)
		(width 0.75)
		(layer "B.Cu")
		(net 10)
		(uuid "b2140dc6-7898-4939-84ae-5136a4848e80")
	)
	(segment
		(start 203.708 132.588)
		(end 209.804 132.588)
		(width 0.75)
		(layer "B.Cu")
		(net 10)
		(uuid "e071c5a9-0033-45f0-9dff-52502453a155")
	)
	(segment
		(start 197.612 116.332)
		(end 197.612 114.554)
		(width 0.75)
		(layer "B.Cu")
		(net 10)
		(uuid "fae08a89-dd40-4423-9fb8-893b31281d82")
	)
	(segment
		(start 222.01 110.35)
		(end 222.01 122.85)
		(width 0.75)
		(layer "F.Cu")
		(net 11)
		(uuid "3207eb65-0f8d-47cf-99a1-2f490b370ee1")
	)
	(segment
		(start 222.01 122.85)
		(end 222.01 124.192)
		(width 0.75)
		(layer "F.Cu")
		(net 11)
		(uuid "3dba62a8-bb09-455d-811c-8ccb4f7520e0")
	)
	(segment
		(start 222.01 124.192)
		(end 220.472 125.73)
		(width 0.75)
		(layer "F.Cu")
		(net 11)
		(uuid "99a3f481-cea0-4d73-b179-31b92a294e38")
	)
	(via
		(at 220.472 125.73)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(net 11)
		(uuid "b9eccd82-f208-4337-a31a-e0bbb4301429")
	)
	(segment
		(start 220.472 125.73)
		(end 202.184 125.73)
		(width 0.75)
		(layer "B.Cu")
		(net 11)
		(uuid "1d902758-4216-4213-bec7-a6a8cdcc59d6")
	)
	(segment
		(start 201.174 117.354)
		(end 200.152 116.332)
		(width 0.75)
		(layer "B.Cu")
		(net 11)
		(uuid "5e19bde2-ebf4-43fd-997c-286c91216da4")
	)
	(segment
		(start 200.152 116.332)
		(end 200.152 114.554)
		(width 0.75)
		(layer "B.Cu")
		(net 11)
		(uuid "5f0407fd-0778-4934-9f44-a334047ee282")
	)
	(segment
		(start 201.174 124.72)
		(end 201.174 122.539)
		(width 0.75)
		(layer "B.Cu")
		(net 11)
		(uuid "889c289d-87f4-44be-9739-0e9a7006c11a")
	)
	(segment
		(start 202.184 125.73)
		(end 201.174 124.72)
		(width 0.75)
		(layer "B.Cu")
		(net 11)
		(uuid "8cf2d1b5-15bb-475e-b592-c8ac038210e1")
	)
	(segment
		(start 201.174 122.539)
		(end 201.174 117.354)
		(width 0.75)
		(layer "B.Cu")
		(net 11)
		(uuid "a766cc08-d5f6-4a07-be0e-8b8d1919a2bf")
	)
	(segment
		(start 196.088 101.346)
		(end 191.77 101.346)
		(width 0.75)
		(layer "F.Cu")
		(net 12)
		(uuid "28f4c7a8-a7ff-48af-9e45-eeed11521edf")
	)
	(segment
		(start 191.77 101.346)
		(end 184.39 108.726)
		(width 0.75)
		(layer "F.Cu")
		(net 12)
		(uuid "bafd5400-02a4-4da5-b777-ab10e7994df0")
	)
	(segment
		(start 184.39 122.85)
		(end 184.39 110.35)
		(width 0.75)
		(layer "F.Cu")
		(net 12)
		(uuid "c8654530-4abe-4a2e-9485-7337269a937d")
	)
	(segment
		(start 184.39 108.726)
		(end 184.39 110.35)
		(width 0.75)
		(layer "F.Cu")
		(net 12)
		(uuid "dc4bf7bb-d592-4d41-98ab-328be0e11e04")
	)
	(via
		(at 196.088 101.346)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(net 12)
		(uuid "7ec2dd02-b159-4527-a9ab-d552f76e6b06")
	)
	(segment
		(start 198.634 103.892)
		(end 196.088 101.346)
		(width 0.75)
		(layer "B.Cu")
		(net 12)
		(uuid "3bbcad86-ef8f-47d4-bd20-4fa70b66f6be")
	)
	(segment
		(start 195.072 112.776)
		(end 198.634 109.214)
		(width 0.75)
		(layer "B.Cu")
		(net 12)
		(uuid "3e4e7e0c-edb1-471f-9b8b-7570fc11f58e")
	)
	(segment
		(start 198.634 109.214)
		(end 198.634 106.569)
		(width 0.75)
		(layer "B.Cu")
		(net 12)
		(uuid "90fa0200-5c3d-45e8-a37b-fcce8a679dd6")
	)
	(segment
		(start 198.634 106.569)
		(end 198.634 103.892)
		(width 0.75)
		(layer "B.Cu")
		(net 12)
		(uuid "9281d27f-6359-4957-9cea-eb4c69cfa402")
	)
	(segment
		(start 195.072 114.554)
		(end 195.072 112.776)
		(width 0.75)
		(layer "B.Cu")
		(net 12)
		(uuid "e6874a76-d4fe-4039-a905-2bba916de101")
	)
	(segment
		(start 212.344 100.684)
		(end 209.45 97.79)
		(width 0.75)
		(layer "F.Cu")
		(net 13)
		(uuid "60023239-b5f0-4214-a9bd-f9dea047997c")
	)
	(segment
		(start 212.344 104.14)
		(end 212.344 100.684)
		(width 0.75)
		(layer "F.Cu")
		(net 13)
		(uuid "647bbdf9-ded5-4c16-a5d8-76ef7f4dc6d5")
	)
	(segment
		(start 196.95 97.79)
		(end 209.45 97.79)
		(width 0.75)
		(layer "F.Cu")
		(net 13)
		(uuid "909a57f5-302a-4c87-b75d-3c214628d230")
	)
	(via
		(at 212.344 104.14)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(net 13)
		(uuid "ec4e67f9-e3e2-4a3f-b8ec-6a136ec84a91")
	)
	(segment
		(start 202.692 116.332)
		(end 202.692 114.554)
		(width 0.75)
		(layer "B.Cu")
		(net 13)
		(uuid "12639990-6dee-4cea-9e70-29fa61c2a421")
	)
	(segment
		(start 203.7665 117.4065)
		(end 202.692 116.332)
		(width 0.75)
		(layer "B.Cu")
		(net 13)
		(uuid "36a749cb-bbb4-4c18-8043-4f3b680c68ec")
	)
	(segment
		(start 212.344 113.909)
		(end 203.714 122.539)
		(width 0.75)
		(layer "B.Cu")
		(net 13)
		(uuid "8edd0f3c-f4bf-4932-8aca-86539fb4ed96")
	)
	(segment
		(start 203.7665 122.4865)
		(end 203.7665 117.4065)
		(width 0.75)
		(layer "B.Cu")
		(net 13)
		(uuid "c52a88d8-6a3e-4547-b20d-24b3e7e091fa")
	)
	(segment
		(start 212.344 104.14)
		(end 212.344 113.909)
		(width 0.75)
		(layer "B.Cu")
		(net 13)
		(uuid "c6532e15-0382-4de0-81c7-65c1c13ca3cd")
	)
	(segment
		(start 203.714 122.539)
		(end 203.7665 122.4865)
		(width 0.75)
		(layer "B.Cu")
		(net 13)
		(uuid "eb5b524e-b6e2-495c-b59e-b4d0c1d8198e")
	)
	(segment
		(start 191.014 104.4)
		(end 191.014 106.569)
		(width 0.75)
		(layer "B.Cu")
		(net 17)
		(uuid "8b457dca-9bd1-4880-b93a-849838e14368")
	)
	(segment
		(start 199.41 75.692)
		(end 196.85 78.252)
		(width 0.75)
		(layer "B.Cu")
		(net 17)
		(uuid "8e4aac14-4bb4-4437-b56b-bc7464979c11")
	)
	(segment
		(start 196.85 78.252)
		(end 196.85 89.154)
		(width 0.75)
		(layer "B.Cu")
		(net 17)
		(uuid "9592cc04-5e1e-4e8b-8cea-460dd990a6d9")
	)
	(segment
		(start 190.246 103.632)
		(end 191.014 104.4)
		(width 0.75)
		(layer "B.Cu")
		(net 17)
		(uuid "d3eaabfd-4729-48b1-bbdd-60d741006f12")
	)
	(segment
		(start 196.85 89.154)
		(end 190.246 95.758)
		(width 0.75)
		(layer "B.Cu")
		(net 17)
		(uuid "db6abbf7-afcc-4074-bb36-b21eff6238c7")
	)
	(segment
		(start 190.246 95.758)
		(end 190.246 103.632)
		(width 0.75)
		(layer "B.Cu")
		(net 17)
		(uuid "f1a7d016-42b2-4aa4-8339-821e7526a3ec")
	)
	(segment
		(start 222.53 137.022999)
		(end 220.303999 139.249)
		(width 0.75)
		(layer "F.Cu")
		(net 19)
		(uuid "2e9299e9-c89c-482b-a3dd-f0b1a9a2867b")
	)
	(segment
		(start 222.53 132.588)
		(end 222.53 137.022999)
		(width 0.75)
		(layer "F.Cu")
		(net 19)
		(uuid "4f252a5d-5aa1-4d9b-b78b-e4440210c926")
	)
	(segment
		(start 220.303999 139.249)
		(end 219.329 139.249)
		(width 0.75)
		(layer "F.Cu")
		(net 19)
		(uuid "749432d0-172b-4f44-8627-fe8a878fd5d0")
	)
	(segment
		(start 222.504 128.524)
		(end 223.806 129.826)
		(width 0.75)
		(layer "F.Cu")
		(net 20)
		(uuid "36df2ed0-6af1-4639-bcb2-8f9c8d323ce2")
	)
	(segment
		(start 223.806 129.826)
		(end 223.806 137.162627)
		(width 0.75)
		(layer "F.Cu")
		(net 20)
		(uuid "6b24a6f5-16e7-4a53-9ea1-982dd8393c7e")
	)
	(segment
		(start 220.449627 140.519)
		(end 219.329 140.519)
		(width 0.75)
		(layer "F.Cu")
		(net 20)
		(uuid "80e00712-6101-4f7d-959e-13d7650456cf")
	)
	(segment
		(start 223.806 137.162627)
		(end 220.449627 140.519)
		(width 0.75)
		(layer "F.Cu")
		(net 20)
		(uuid "e99c3eac-1d91-40eb-9aaf-155a9ba2aa7d")
	)
	(segment
		(start 210.566 141.276)
		(end 212.593 139.249)
		(width 0.75)
		(layer "F.Cu")
		(net 21)
		(uuid "6254eaea-5f4f-4396-9570-8a556e4bebfd")
	)
	(segment
		(start 212.593 139.249)
		(end 214.379 139.249)
		(width 0.75)
		(layer "F.Cu")
		(net 21)
		(uuid "828fd899-7752-40bc-ad60-8d4f028f8d6c")
	)
	(segment
		(start 212.658 143.51)
		(end 214.379 141.789)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "24b9b497-f7f7-42ff-a294-a607d8df017d")
	)
	(segment
		(start 213.6505 128.524)
		(end 213.6505 132.588)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "43992bee-8923-4efb-a0b3-9fe6cde72df3")
	)
	(segment
		(start 219.456 136.144)
		(end 219.329 136.271)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "738c711a-50cf-4e57-9432-1f48a75613c9")
	)
	(segment
		(start 219.329 136.271)
		(end 219.329 137.979)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "ab90da9d-7f5b-4841-905c-8629d55db97b")
	)
	(segment
		(start 219.456 135.382)
		(end 216.4445 135.382)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "d209da73-cf28-4cdc-88a3-14cad701502b")
	)
	(segment
		(start 219.456 135.382)
		(end 219.456 136.144)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "dd29bd75-0150-42b8-b465-833fd45a5e11")
	)
	(segment
		(start 210.566 143.51)
		(end 212.658 143.51)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "f8ecd635-f873-4786-a7f7-9d3a29fa2008")
	)
	(segment
		(start 216.4445 135.382)
		(end 213.6505 132.588)
		(width 0.75)
		(layer "F.Cu")
		(net 22)
		(uuid "fb5006d4-68f4-4ea2-959b-2478c61cd16c")
	)
	(via
		(at 219.456 135.382)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(net 22)
		(uuid "884a757b-5cad-49e3-8c6f-2b49944934e8")
	)
	(via
		(at 210.566 143.51)
		(size 2.3)
		(drill 1)
		(layers "F.Cu" "B.Cu")
		(net 22)
		(uuid "928ba6b1-5590-4357-ad59-b259e8c6091a")
	)
	(segment
		(start 210.566 143.51)
		(end 216.88 143.51)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "294d2b6d-ca2d-4c58-8ed8-6de54365a822")
	)
	(segment
		(start 207.296885 143.51)
		(end 204.72 140.933115)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "2e9ac9a9-b41f-4559-bdba-5ff8cc266a55")
	)
	(segment
		(start 204.72 138.634)
		(end 204.72 137.89)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "3717b4f1-5bdf-429b-bdc2-e29c33b366f6")
	)
	(segment
		(start 202.108 139.116)
		(end 204.238 139.116)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "48b2a87e-682b-44d9-b438-68e9e83c1d81")
	)
	(segment
		(start 204.72 140.933115)
		(end 204.72 137.89)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "6774e689-97eb-4030-8b2d-c7662a46b243")
	)
	(segment
		(start 219.456 140.934)
		(end 219.456 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "7e4d07bb-d2f8-4a22-9f4b-58f5790820f8")
	)
	(segment
		(start 210.566 143.51)
		(end 207.296885 143.51)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "92bf8bb1-6f97-4336-a70a-543f55d44c29")
	)
	(segment
		(start 204.238 139.116)
		(end 204.72 138.634)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "9d982b7f-71c9-4691-b317-07d8305cf575")
	)
	(segment
		(start 201.68 138.688)
		(end 202.108 139.116)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "a9234ca3-f1bd-452d-8568-27cf35df8da8")
	)
	(segment
		(start 216.88 143.51)
		(end 219.456 140.934)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "de74b6a4-cfde-437d-952a-3109e04dcaf5")
	)
	(segment
		(start 201.68 137.89)
		(end 201.68 138.688)
		(width 0.75)
		(layer "B.Cu")
		(net 22)
		(uuid "f58f3530-ce7d-4c4c-8dea-6446593cb59b")
	)
	(segment
		(start 195.808 141.224)
		(end 195.834 141.25)
		(width 0.75)
		(layer "F.Cu")
		(net 24)
		(uuid "4399cb4f-070a-4034-af20-e79784619b02")
	)
	(segment
		(start 193.4155 141.224)
		(end 195.808 141.224)
		(width 0.75)
		(layer "F.Cu")
		(net 24)
		(uuid "7c241aea-6279-4d4a-b783-d114bdc75c04")
	)
	(segment
		(start 190.5 138.8995)
		(end 188.976 140.4235)
		(width 0.75)
		(layer "F.Cu")
		(net 25)
		(uuid "0e605b26-c132-4df5-99ab-1edbed14ff76")
	)
	(segment
		(start 189.7765 141.224)
		(end 191.1405 141.224)
		(width 0.5)
		(layer "F.Cu")
		(net 25)
		(uuid "46b43f7a-e484-4671-a98c-9f4225f232ff")
	)
	(segment
		(start 188.976 140.4235)
		(end 189.7765 141.224)
		(width 0.5)
		(layer "F.Cu")
		(net 25)
		(uuid "760521d5-1d2a-4f85-a4a3-0dc9dc0ae7e4")
	)
	(segment
		(start 190.5 138.176)
		(end 190.5 138.8995)
		(width 0.75)
		(layer "F.Cu")
		(net 25)
		(uuid "d28cda51-9de2-475d-a5f8-faf5db1b4768")
	)
	(segment
		(start 216.6255 128.524)
		(end 219.404 128.524)
		(width 0.75)
		(layer "F.Cu")
		(net 26)
		(uuid "397f81b8-f363-499d-aee3-80704f92f324")
	)
	(segment
		(start 216.6255 132.588)
		(end 219.43 132.588)
		(width 0.75)
		(layer "F.Cu")
		(net 27)
		(uuid "62195978-3d94-457b-9d28-41ee7a849f92")
	)
	(segment
		(start 202.7 135.872)
		(end 202.21 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 28)
		(uuid "9f6abdec-2e0c-45bd-a44a-bef44d00d252")
	)
	(segment
		(start 202.7 137.89)
		(end 202.7 135.872)
		(width 0.75)
		(layer "B.Cu")
		(net 28)
		(uuid "b19d1030-c69b-4923-8868-ed3aaa04cec8")
	)
	(segment
		(start 203.7 137.89)
		(end 203.7 135.872)
		(width 0.75)
		(layer "B.Cu")
		(net 29)
		(uuid "4be2abbe-597e-4997-aa14-5ecf045ebbf9")
	)
	(segment
		(start 203.7 135.872)
		(end 204.19 135.382)
		(width 0.75)
		(layer "B.Cu")
		(net 29)
		(uuid "a3e4578a-7641-4493-bf80-ff6e831dd95f")
	)
	(segment
		(start 186.944 130.81)
		(end 185.166 130.81)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "1e3095f2-f546-4b66-9eaa-a685bd67ab9d")
	)
	(segment
		(start 188.976 143.5485)
		(end 188.976 143.256)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "225a28c0-65fe-4936-a5ae-02ce35104b1b")
	)
	(segment
		(start 188.448 132.314)
		(end 186.944 130.81)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "5624402e-47bc-44ec-ba62-721e9d35f694")
	)
	(segment
		(start 188.448 133.0885)
		(end 188.448 132.314)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "5b2e922f-bf9e-4914-a6a3-da0644403319")
	)
	(segment
		(start 183.134 139.446)
		(end 184.624197 140.936197)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "5be9ec85-9e04-4c77-a946-afe55705d26f")
	)
	(segment
		(start 183.134 132.842)
		(end 183.134 139.446)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "5d1b0923-3596-4afa-aefa-13acaa1a5085")
	)
	(segment
		(start 185.166 130.81)
		(end 183.134 132.842)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "64085cba-160e-425c-b7e8-671c8c302fa0")
	)
	(segment
		(start 184.624197 140.936197)
		(end 185.707803 140.936197)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "8c39f444-e023-47dd-bc96-45d79d5a19eb")
	)
	(segment
		(start 190.058 142.174)
		(end 191.1405 142.174)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "b9da840e-b65b-494c-a1b8-c5000cf2bd30")
	)
	(segment
		(start 186.656197 140.936197)
		(end 188.976 143.256)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "d0520898-e834-452e-84a6-6914ea1aa0b7")
	)
	(segment
		(start 188.976 143.256)
		(end 190.058 142.174)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "daf7f3e9-6f7d-459a-ae33-2b4c96d9ced8")
	)
	(segment
		(start 185.707803 140.936197)
		(end 185.823 141.051394)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "e3d8a38a-7273-46a2-9d36-3d0dc4e86adc")
	)
	(segment
		(start 185.707803 140.936197)
		(end 186.656197 140.936197)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "f8f5ec3f-4f6f-47ac-b650-7698acea4bf3")
	)
	(segment
		(start 185.823 141.051394)
		(end 185.823 143.85)
		(width 0.75)
		(layer "F.Cu")
		(net 30)
		(uuid "f8fc9fcd-d2d1-454b-9a9c-6d5cd5307b9b")
	)
	(segment
		(start 207.01 98.806)
		(end 219.456 98.806)
		(width 0.75)
		(layer "B.Cu")
		(net 31)
		(uuid "45bac9a8-160b-430d-b117-93c06bad6eb7")
	)
	(segment
		(start 201.174 106.569)
		(end 201.174 104.642)
		(width 0.75)
		(layer "B.Cu")
		(net 31)
		(uuid "8f636c15-d629-46fc-9c32-e2c7c90d9d82")
	)
	(segment
		(start 219.456 98.806)
		(end 219.964 98.298)
		(width 0.75)
		(layer "B.Cu")
		(net 31)
		(uuid "dbb45d5f-3f9e-4edc-abeb-7d4486430bc1")
	)
	(segment
		(start 201.174 104.642)
		(end 207.01 98.806)
		(width 0.75)
		(layer "B.Cu")
		(net 31)
		(uuid "f955c22a-e100-4326-83a5-72b1bfe40e49")
	)
	(segment
		(start 203.714 106.569)
		(end 203.714 104.134)
		(width 0.75)
		(layer "B.Cu")
		(net 32)
		(uuid "47eba028-cdac-4f0a-9c95-47bf8740cc78")
	)
	(segment
		(start 207.518 100.33)
		(end 219.456 100.33)
		(width 0.75)
		(layer "B.Cu")
		(net 32)
		(uuid "56958c3b-3d8a-4bc7-a618-7c06fe551e67")
	)
	(segment
		(start 219.456 100.33)
		(end 219.964 100.838)
		(width 0.75)
		(layer "B.Cu")
		(net 32)
		(uuid "79be51bb-2327-4dc3-af95-3f9637d55da6")
	)
	(segment
		(start 203.714 104.134)
		(end 207.518 100.33)
		(width 0.75)
		(layer "B.Cu")
		(net 32)
		(uuid "a4e9e2e4-6fce-4342-bdc3-4c0b3d7244e1")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(uuid "bb822890-b771-4542-8ef6-a0d91ba779cd")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 196.209 129.177838) (xy 195.459 129.177838) (xy 194.834 130.769728) (xy 195.834 131.319) (xy 196.834 130.769728)
			)
		)
		(filled_polygon
			(layer "F.Cu")
			(pts
				(xy 196.209 129.177838) (xy 195.459 129.177838) (xy 194.834 130.769728) (xy 195.834 131.319) (xy 196.834 130.769728)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "0403e150-e594-4c04-9582-53c221305ff8")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.27495 125.051279) (xy 188.805279 124.52095) (xy 189.236 124.0515) (xy 188.473293 122.538293)
				(xy 187.75594 124.0515)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 188.27495 125.051279) (xy 188.805279 124.52095) (xy 189.236 124.0515) (xy 188.473293 122.538293)
				(xy 187.75594 124.0515)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Net-(J1-Pin_2)")
		(layer "B.Cu")
		(uuid "1302ce15-9d41-4d93-a293-71b3a6886ca7")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 217.940749 99.955) (xy 217.940749 100.705) (xy 219.187444 101.673876) (xy 219.965 100.838) (xy 219.676622 99.73462)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 217.940749 99.955) (xy 217.940749 100.705) (xy 219.187444 101.673876) (xy 219.965 100.838) (xy 219.676622 99.73462)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(J3-Pin_3)")
		(layer "B.Cu")
		(uuid "1821e7ce-2e58-439f-ba36-6a42664763bf")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 200.97495 125.051279) (xy 201.505279 124.52095) (xy 201.936 124.0515) (xy 201.173293 122.538293)
				(xy 200.45594 124.0515)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 200.97495 125.051279) (xy 201.505279 124.52095) (xy 201.936 124.0515) (xy 201.173293 122.538293)
				(xy 200.45594 124.0515)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(J3-Pin_5)")
		(layer "B.Cu")
		(uuid "243fcf71-90e2-428a-b027-597d5960aa73")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 198.259 108.8435) (xy 199.009 108.8435) (xy 199.396 108.0815) (xy 198.634 106.568) (xy 197.872 108.0815)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 198.259 108.8435) (xy 199.009 108.8435) (xy 199.396 108.0815) (xy 198.634 106.568) (xy 197.872 108.0815)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+3.3V")
		(layer "B.Cu")
		(uuid "273578dc-781a-4b4e-81da-c7599a7ba6fc")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 207.385 85.05) (xy 206.635 85.05) (xy 206.01 86.05) (xy 207.01 87.151) (xy 208.01 86.05)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 207.385 85.05) (xy 206.635 85.05) (xy 206.01 86.05) (xy 207.01 87.151) (xy 208.01 86.05)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(J3-Pin_5)")
		(layer "B.Cu")
		(uuid "2975c7ec-aa0a-45f1-ad77-b4802e0e2675")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.593252 112.785077) (xy 195.062923 112.254748) (xy 194.149607 113.871307) (xy 195.071293 114.554707)
				(xy 196.134461 114.113914)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 195.593252 112.785077) (xy 195.062923 112.254748) (xy 194.149607 113.871307) (xy 195.071293 114.554707)
				(xy 196.134461 114.113914)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "297ede01-8c0a-4e84-8579-1e4908564c38")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 204.301117 89.515446) (xy 204.831446 88.985117) (xy 205.493797 87.657052) (xy 204.469293 87.149293)
				(xy 203.495619 87.742646)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 204.301117 89.515446) (xy 204.831446 88.985117) (xy 205.493797 87.657052) (xy 204.469293 87.149293)
				(xy 203.495619 87.742646)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(J1-Pin_3)")
		(layer "B.Cu")
		(uuid "2f4d4c60-8e45-4d6c-b489-b2ade8eefc25")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.684884 104.661445) (xy 201.154555 104.131116) (xy 200.577981 105.0565) (xy 201.173293 106.569707)
				(xy 201.936 105.0565)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 201.684884 104.661445) (xy 201.154555 104.131116) (xy 200.577981 105.0565) (xy 201.173293 106.569707)
				(xy 201.936 105.0565)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(J3-Pin_3)")
		(layer "B.Cu")
		(uuid "39a3d73b-b9cf-40e2-a9f4-7468ef4abc39")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 200.142923 116.853252) (xy 200.673252 116.322923) (xy 201.214461 114.994086) (xy 200.151293 114.553293)
				(xy 199.229607 115.236692)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 200.142923 116.853252) (xy 200.673252 116.322923) (xy 201.214461 114.994086) (xy 200.151293 114.553293)
				(xy 199.229607 115.236692)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(DS1-SCK)")
		(layer "B.Cu")
		(uuid "3a38c68f-3527-47d1-9675-a6f5a6abb9a9")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.568554 88.985117) (xy 202.098883 89.515446) (xy 202.90438 87.742645) (xy 201.930707 87.149293)
				(xy 200.906202 87.657053)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 201.568554 88.985117) (xy 202.098883 89.515446) (xy 202.90438 87.742645) (xy 201.930707 87.149293)
				(xy 200.906202 87.657053)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(J3-Pin_2)")
		(layer "B.Cu")
		(uuid "49acce00-0f81-4e78-a00c-f527ea6a1556")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 205.27998 121.50335) (xy 204.74965 120.97302) (xy 204.14887 121.0265) (xy 203.713293 122.539707)
				(xy 204.476 122.85463)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 205.27998 121.50335) (xy 204.74965 120.97302) (xy 204.14887 121.0265) (xy 203.713293 122.539707)
				(xy 204.476 122.85463)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(DS1-SDA)")
		(layer "B.Cu")
		(uuid "4f8044dd-75e2-48e0-9e49-e9690981d249")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 193.488807 104.058478) (xy 192.958478 104.588807) (xy 192.792 105.0565) (xy 193.554707 106.569707)
				(xy 194.101897 105.0565)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 193.488807 104.058478) (xy 192.958478 104.588807) (xy 192.792 105.0565) (xy 193.554707 106.569707)
				(xy 194.101897 105.0565)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(J3-Pin_5)")
		(layer "B.Cu")
		(uuid "5060bc8e-c444-4560-a315-69b48b3f85d9")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 199.009 104.2945) (xy 198.259 104.2945) (xy 197.872 105.0565) (xy 198.634 106.57) (xy 199.396 105.0565)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 199.009 104.2945) (xy 198.259 104.2945) (xy 197.872 105.0565) (xy 198.634 106.57) (xy 199.396 105.0565)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "533717af-e731-48ea-92cb-cfbaed85c124")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 204.845 85.009838) (xy 204.095 85.009838) (xy 203.47 86.601728) (xy 204.47 87.151) (xy 205.47 86.601728)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 204.845 85.009838) (xy 204.095 85.009838) (xy 203.47 86.601728) (xy 204.47 87.151) (xy 205.47 86.601728)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "718c340d-3302-4983-9256-7489ebf92497")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.663473 129.093143) (xy 195.133143 129.623473) (xy 194.771539 130.877914) (xy 195.834707 131.318707)
				(xy 196.690823 130.562391)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 195.663473 129.093143) (xy 195.133143 129.623473) (xy 194.771539 130.877914) (xy 195.834707 131.318707)
				(xy 196.690823 130.562391)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(J3-Pin_4)")
		(layer "B.Cu")
		(uuid "72c4e862-9265-4a4a-8c8a-0e14afa3e13e")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 197.090748 116.322923) (xy 197.621077 116.853252) (xy 198.534392 115.236692) (xy 197.612707 114.553293)
				(xy 196.549539 114.994086)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 197.090748 116.322923) (xy 197.621077 116.853252) (xy 198.534392 115.236692) (xy 197.612707 114.553293)
				(xy 196.549539 114.994086)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+3.3V")
		(layer "B.Cu")
		(uuid "88415c01-45e0-470a-bc88-9b6f6b8d83ac")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.389 120.2645) (xy 190.639 120.2645) (xy 190.252 121.0265) (xy 191.014 122.54) (xy 191.776 121.0265)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 191.389 120.2645) (xy 190.639 120.2645) (xy 190.252 121.0265) (xy 191.014 122.54) (xy 191.776 121.0265)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "8a7f63cd-dee5-4651-a42b-4a64f4aa97bc")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 218.422059 102.321729) (xy 217.891729 102.852059) (xy 218.864 103.988317) (xy 219.964707 103.378707)
				(xy 218.864 102.278)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 218.422059 102.321729) (xy 217.891729 102.852059) (xy 218.864 103.988317) (xy 219.964707 103.378707)
				(xy 218.864 102.278)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(J3-Pin_4)")
		(layer "B.Cu")
		(uuid "94a40ea2-7233-4cc4-9a77-97ae196a8f82")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 196.469 120.2645) (xy 195.719 120.2645) (xy 195.332 121.0265) (xy 196.094 122.54) (xy 196.856 121.0265)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 196.469 120.2645) (xy 195.719 120.2645) (xy 195.332 121.0265) (xy 196.094 122.54) (xy 196.856 121.0265)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(J3-Pin_3)")
		(layer "B.Cu")
		(uuid "995012e3-2782-4719-8b0a-7697dbe4b5db")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.549 120.2645) (xy 200.799 120.2645) (xy 200.412 121.0265) (xy 201.174 122.54) (xy 201.936 121.0265)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 201.549 120.2645) (xy 200.799 120.2645) (xy 200.412 121.0265) (xy 201.174 122.54) (xy 201.936 121.0265)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "9c84c3c8-ba7c-429e-ab3c-49354036c79a")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 222.036271 102.852059) (xy 221.505941 102.321729) (xy 221.064 102.278) (xy 219.963293 103.378707)
				(xy 221.064 103.988317)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 222.036271 102.852059) (xy 221.505941 102.321729) (xy 221.064 102.278) (xy 219.963293 103.378707)
				(xy 221.064 103.988317)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(DS1-SCK)")
		(layer "B.Cu")
		(uuid "a5db2909-78c6-4e21-a17a-067c6b11f2d8")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.925356 104.209025) (xy 195.395025 104.739356) (xy 195.332 105.0565) (xy 196.094707 106.569707)
				(xy 196.559145 105.0565)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 195.925356 104.209025) (xy 195.395025 104.739356) (xy 195.332 105.0565) (xy 196.094707 106.569707)
				(xy 196.559145 105.0565)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(J1-Pin_3)")
		(layer "B.Cu")
		(uuid "a8578b8e-5e76-46cc-ae08-ba12468d357a")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 217.940749 98.431) (xy 217.940749 99.181) (xy 219.676622 99.401379) (xy 219.965 98.298) (xy 219.187444 97.462123)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 217.940749 98.431) (xy 217.940749 99.181) (xy 219.676622 99.401379) (xy 219.965 98.298) (xy 219.187444 97.462123)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+BATT")
		(layer "B.Cu")
		(uuid "ab24e0a5-37aa-457b-a0c6-226e7a813442")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.559 124.8135) (xy 186.309 124.8135) (xy 186.696 124.0515) (xy 185.934 122.538) (xy 185.172 124.0515)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 185.559 124.8135) (xy 186.309 124.8135) (xy 186.696 124.0515) (xy 185.934 122.538) (xy 185.172 124.0515)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "b00d9cb8-daa0-4558-a74b-3c7a6866ef7a")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 219.589 105.478) (xy 220.339 105.478) (xy 220.964 104.478) (xy 219.964 103.377) (xy 218.964 104.478)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 219.589 105.478) (xy 220.339 105.478) (xy 220.964 104.478) (xy 219.964 103.377) (xy 218.964 104.478)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(J3-Pin_2)")
		(layer "B.Cu")
		(uuid "b1125b75-3f2d-4708-a38f-08ba0994b9da")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 202.682923 116.853252) (xy 203.213252 116.322923) (xy 203.754461 114.994086) (xy 202.691293 114.553293)
				(xy 201.769607 115.236692)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 202.682923 116.853252) (xy 203.213252 116.322923) (xy 203.754461 114.994086) (xy 202.691293 114.553293)
				(xy 201.769607 115.236692)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(BZ1-+)")
		(layer "B.Cu")
		(uuid "b7dc6dbd-9e74-4cdb-ad9c-e6ce8a8f3e9d")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.204565 104.060236) (xy 190.674236 104.590565) (xy 190.252 105.0565) (xy 191.014707 106.569707)
				(xy 191.726361 105.0565)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 191.204565 104.060236) (xy 190.674236 104.590565) (xy 190.252 105.0565) (xy 191.014707 106.569707)
				(xy 191.726361 105.0565)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "bdda7fb1-3b75-4dd1-b2cd-6f1d61cb7035")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.133143 133.012527) (xy 195.663473 133.542857) (xy 196.690823 132.073608) (xy 195.834707 131.317293)
				(xy 194.771539 131.758086)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 195.133143 133.012527) (xy 195.663473 133.542857) (xy 196.690823 132.073608) (xy 195.834707 131.317293)
				(xy 194.771539 131.758086)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(J3-Pin_4)")
		(layer "B.Cu")
		(uuid "d5e36e15-0da9-4fc9-b0b9-5b2dc3f961c8")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.719 124.8135) (xy 196.469 124.8135) (xy 196.856 124.0515) (xy 196.094 122.538) (xy 195.332 124.0515)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 195.719 124.8135) (xy 196.469 124.8135) (xy 196.856 124.0515) (xy 196.094 122.538) (xy 195.332 124.0515)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(uuid "dac8d22d-29ed-4007-ae3f-c173f4f8fc92")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 207.304271 113.012059) (xy 206.773941 112.481729) (xy 204.917786 113.454) (xy 205.231293 114.554707)
				(xy 206.332 114.868214)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 207.304271 113.012059) (xy 206.773941 112.481729) (xy 204.917786 113.454) (xy 205.231293 114.554707)
				(xy 206.332 114.868214)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Net-(J1-Pin_2)")
		(layer "B.Cu")
		(uuid "e450dbd8-2f5f-434e-a0dd-2e6635091693")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 204.089 104.2945) (xy 203.339 104.2945) (xy 202.952 105.0565) (xy 203.714 106.57) (xy 204.476 105.0565)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 204.089 104.2945) (xy 203.339 104.2945) (xy 202.952 105.0565) (xy 203.714 106.57) (xy 204.476 105.0565)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(DS1-SDA)")
		(layer "B.Cu")
		(uuid "ea565edd-4633-4798-bad0-51b5493f086f")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 199.028554 88.985117) (xy 199.558883 89.515446) (xy 200.36438 87.742645) (xy 199.390707 87.149293)
				(xy 198.366202 87.657053)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 199.028554 88.985117) (xy 199.558883 89.515446) (xy 200.36438 87.742645) (xy 199.390707 87.149293)
				(xy 198.366202 87.657053)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(J3-Pin_2)")
		(layer "B.Cu")
		(uuid "ede71c28-6b2a-4369-9ee7-7f991e31708a")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 204.1415 120.2645) (xy 203.3915 120.2645) (xy 202.986717 121.0265) (xy 203.714 122.54) (xy 204.476 121.0265)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 204.1415 120.2645) (xy 203.3915 120.2645) (xy 202.986717 121.0265) (xy 203.714 122.54) (xy 204.476 121.0265)
			)
		)
	)
	(embedded_fonts no)
)
